For 1990-2009 cars

1. Inspect the transaxle wiring harness assembly (224) for:

• | Cut or pinched wires

• | Cut wire insulation

• | Bent or broken electrical connectors

• | Damaged terminal pins

2. Position the wire harness assembly (224) onto the valve body (300) and pump assembly (200).
3. Mate each connector into its respective electrical component and engage the locking tabs.
4. Secure the harness conduit into the retaining clip (226) on the oil pump cover (201).
5. Assemble the automatic transaxle temperature sensor (391) into the retaining clip (390).