For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable to Battery Post | 15 N·m | 11 lb ft
Battery Cable to Generator Output Stud | 20 N·m | 15 lb ft
Battery Cable to Starter | 10 N·m | 85 lb in
Battery Hold Down Retainer Bolt | 18 N·m | 13 lb ft
Generator Mounting Bolt | 50 N·m | 37 lb ft
Generator Output Wire Retainer | 20 N·m | 15 lb ft
ICM Nut | 8 N·m | 70 lb in
Ignition Coil Screw | 4-5 N·m | 40 lb in
Positive Booster Cable Bolt at Multifuse Relay Center | 10 N·m | 85 lb in
Rear Pencil Brace Bolt | 30 N·m | 22 lb ft
Solenoid Battery Terminal Nut | 16 N·m | 12 lb ft
Solenoid Screw | 6.5 N·m | 60 lb in
Solenoid S Terminal Nut | 2.5 N·m | 22 lb in
Spark Plug | 15 N·m | 11 lb ft
Starter Motor Mounting Bolt | 43 N·m | 32 lb ft