For 1990-2009 cars

### Removal Procedure

1. Remove the push-pin (3) from the rail mounted assist handle.
2. Remove the fasteners from under the assist handle (1).
3. Remove the assist handle from the headliner.
4. Disconnect the wiring harness connector, if equipped.

### Installation Procedure

1. Connect the wiring harness connector, if equipped.
2. Align the following components:

• | The assist handle

• | The headliner opening

• | The retainer behind the headliner

3. Install the fasteners.
4. Press the push-pin (3) into place.