For 1990-2009 cars

### Removal Procedure

1. Release the retainers at the top of the door lock switch bezel.

Use a small, flat-bladed tool.

2. Pull outward the inside door handle.
3. Remove the bezel.

Lift the bezel upward over the inside door handle.

4. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.
2. Engage the lower tabs on the bezel to the trim panel.
3. Align the lock rod with the lock rod knob.
4. Install the bezel to the trim panel.