For 1990-2009 cars

### Removal Procedure

1. Remove the left sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.
2. Disconnect the vacuum hose from the outside air/recirculation actuator (1).
3. Unclip the outside air/recirculation actuator (1) from the air inlet.
4. Disengage the outside air/recirculation actuator (1) from the valve.

### Installation Procedure

1. Engage the outside air/recirculation actuator (1) to the valve.
2. Clip the outside air/recirculation actuator (1) to the air inlet.
3. Connect the vacuum hose to the outside air/recirculation actuator (1).

Install the left sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.