For 1990-2009 cars

## Radio Rear Speaker Grille Replacement Pontiac with UZ8

### Removal Procedure

1. Carefully pry up on the front of the speaker grille assembly to disengage the retainers.

Slide the grille forward to disengage the retaining hooks (1).

2. Partially remove the grille assembly.

Disconnect the electrical connector (3).

3. Remove the speaker grille.
4. Remove the speaker from the grille if necessary. Refer to Speaker Replacement .

### Installation Procedure

1. Install the speaker to the grille if necessary. Refer to Speaker Replacement .
2. Partially install the speaker grille.

Connect the electrical connector (3).

3. Slide the rear of the speaker grille retaining hooks (1) on to the rear shelf panel.
4. Align the retaining studs (1) on the front of the speaker grille to the retainers (2) in the shelf panel.

Push downward in order to secure the speaker grille.

## Radio Rear Speaker Grille Replacement Pontiac with UW6/UX7

### Removal Procedure

1. Carefully pry up on the speaker grille (1) in order to disengage the tabs.
2. Remove the speaker grille.

### Installation Procedure

Important: Insert tab with 3 notches on side of grille to outboard slot on trim panel.

1. Install the grille (1) to the trim panel.

Align the tabs.

2. Push downward in order to secure the grille to the trim panel.