For 1990-2009 cars

## Electronic Traction Control Switch Replacement Oldsmobile

### Removal Procedure

1. Remove the knee bolster. Refer to Instrument Panel Knee Bolster .
2. Disengage the retainers fastening the traction control switch (4).

Remove the switch.

### Installation Procedure

1. Install the switch (4) to the knee bolster.
2. Install the knee bolster. Refer to Instrument Panel Knee Bolster .

## Electronic Traction Control Switch Replacement Pontiac

To service the traction control switch refer to Front Floor Console Side Trim Panel Replacement - Left Side .

## Electronic Traction Control Switch Replacement Buick

To service the traction control switch refer to Instrument Panel Multifunction Switch Assembly Replacement .