For 1990-2009 cars

The services shown in this schedule up to 166 000 km (100,000 mi) should be preformed after 166 000 km (100,000 mi) at the same intervals. The services shown at 240 000 km (150,000 mi) should be preformed at the same interval after 240 000 km (150,000 mi).

### Footnotes

[Dagger] The U.S. Environmental Protection Agency or the California Air Resources Board has determined that the failure to perform this maintenance item will not nullify the emission warranty or limit recall liability prior to the completion of the vehicle's useful life. We, however, urge that all recommended maintenance services be performed at the indicated intervals and the maintenance be recorded.

# Lubricate the grease fittings in the suspension and steering linkage, the transaxle shift linkage, parking brake cable guides and underbody contact points and linkage.

* If this vehicle is equipped with an Oil Life Indicator. This feature will let you know when to change the oil and filter -- usually between 3,000 miles (5 000 km) and 7,500 miles (12 500 km) since your last oil change. Under severe conditions, the indicator may come on before 3,000 miles (5 000 km). For description and resetting information, refer to Oil Life Indicator.

+ A good time to check your brakes is during tire rotation. Refer to Brake System Inspection.

#### 5 000 km (3,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 10 500 km (6,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 15 000 km (9,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 20 500 km (12,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 25 000 km (15,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Inspect air cleaner filter if you are driving in dusty conditions. Replace filter if necessary.

| An Emission Control Service. See footnote [Dagger].

#### 30 000 km (18,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 35 000 km (21,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 40 000 km (24,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 45 000 km (27,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 50 000 km (30,000 miles)

• | Check Oil Life Indicator. If engine oil and filter are changed, reset the Oil Life Indicator. Refer to Oil Life Indicator.

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Replace air cleaner filter.

| An Emission Control Service.

• | Inspect fuel tank, cap and lines for damage or leaks. Inspect fuel cap gasket for any damage. Replace parts as needed.

| An Emission Control Service. See footnote [Dagger].

• | For supercharged engines only: Check the supercharger oil level and add oil as needed (or every 36 months, whichever occurs first). Refer to Recommended Fluids and lubricants.

| An Emission Control Service. See footnote [Dagger].

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 55 000 km (33,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 60 000 km (36,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 65 000 km (39,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 70 000 km (42,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 75 000 km (45,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Inspect air cleaner filter if you are driving in dusty conditions. Replace filter if necessary.

| An Emission Control Service. See footnote [Dagger].

#### 80 000 km (48,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 83 000 km (50,000 miles)

• | Change the automatic transmission fluid and filter if the vehicle is mainly driven under one or more of these conditions:

- | In heavy city traffic where the outside temperature regularly reaches 90°F (32°C) or higher.

- | In hilly or mountainous terrain.

- | When doing frequent trailer towing.

- | Uses such as found in taxi, police or delivery service.

• | If the vehicle is not used under any of these conditions, the automatic transmission fluid and filter do not require a change.

#### 85 000 km (51,000 Miles)

Change engine oil and filter (or every 3 Months, whichever occurs first).

An Emission Control Service.

#### 90 000 km (54,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 95 000 km (57,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 100 000 km (60,000 miles)

• | Check Oil Life Indicator. If engine oil and filter are changed, reset the Oil Life Indicator. Refer to Oil Life Indicator.

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Inspect engine accessory drive belt.

| An Emission Control Service.

• | Replace air cleaner filter.

| An Emission Control Service.

• | Inspect fuel tank, cap and lines for damage or leaks. Inspect fuel cap gasket for any damage. Replace parts as needed.

| An Emission Control Service. See footnote [Dagger].

• | For supercharged engines only: Check the supercharger oil level and add oil as needed (or every 36 months, whichever occurs first). Refer to Recommended Fluids and lubricants.

| An Emission Control Service. See footnote [Dagger].

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 105 000 km (63,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 110 000 km (66,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 115 000 km (69,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 120 000 km (72,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 125 000 km (75,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Inspect air cleaner filter if you are driving in dusty conditions. Replace filter if necessary.

| An Emission Control Service. See footnote [Dagger].

#### 130 000 km (78,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 135 000 km (81,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 140 000 km (84,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 145 000 km (87,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 150 000 km (90,000 miles)

• | Check Oil Life Indicator. If engine oil and filter are changed, reset the Oil Life Indicator. Refer to Oil Life Indicator.

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Replace air cleaner filter.

| An Emission Control Service.

• | Inspect fuel tank, cap and lines for damage or leaks. Inspect fuel cap gasket for any damage. Replace parts as needed.

| An Emission Control Service. See footnote [Dagger].

• | For supercharged engines only: Check the supercharger oil level and add oil as needed (or every 36 months, whichever occurs first). Refer to Recommended Fluids and lubricants.

| An Emission Control Service. See footnote [Dagger].

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 155 000 km (93,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 160 000 km (96,000 miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

| An Emission Control Service.

• | Lubricate chassis components (or every 6 months, which ever occurs first). See footnote #.

• | Rotate tires. Refer to Tire Inspection and Rotation for proper rotation pattern and additional information. See footnote +.

#### 165 000 km (99,000 miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

An Emission Control Service.

#### 166 000 km (100,000 miles)

• | Inspect spark plug wires.

| An Emission Control Service.

• | Replace spark plugs.

| An Emission Control Service.

• | Change the automatic transmission fluid and filter if the vehicle is mainly driven under one or more of these conditions:

- | In heavy city traffic where the outside temperature regularly reaches 90°F (32°C) or higher.

- | In hilly or mountainous terrain.

- | When doing frequent trailer towing.

- | Uses such as found in taxi, police or delivery service.

• | If the vehicle is not used under any of these conditions, the automatic transmission fluid and filter do not require a change.

#### 240 000 km (150,000 miles)

Drain, flush and refill the cooling system (or every 60 months since the last cooling system service, whichever occurs first). For information on the proper coolant to use, refer to Engine Coolant. Inspect hoses. Clean radiator, condenser, pressure cap and neck. Pressure test the cooling system and pressure cap.

An Emission Control Service.