For 1990-2009 cars

### Removal Procedure

1. Remove the pump assembly from the vehicle, if necessary for access.
2. Protect the drive shaft with the shim stock.
3. Use a small chisel in order to remove the seal.
4. Discard the seal.

### Installation Procedure

1. Lubricate the new drive shaft seal with power steering fluid.
2. Use the J 7728 in order to install the new drive shaft seal.
3. Install the pump assembly to the vehicle, if removed.