For 1990-2009 cars

## Defroster Grille Replacement Oldsmobile/Pontiac

### Removal Procedure

1. Pry upward in order to remove the windshield defroster grille from the IP.
2. Disconnect the sensors, if equipped. Refer to Sunload and Twilight Sentinel Sensor Replacement .
3. Remove the defroster grille.

### Installation Procedure

1. Partially install the defroster grille.
2. Install the sensors into the defroster grille. Refer to Sunload and Twilight Sentinel Sensor Replacement .
3. Insert the forward edge.
4. Press the rear edge into position.

## Defroster Grille Replacement Buick

The defroster grille is part of the IP upper trim panel to service the defroster grille. Refer to Instrument Panel Upper Trim Pad Replacement .