For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Set the valet switch to the UNLOCK position.
2. Press the rear compartment lid release switch mounted on the instrument panel.

The rear compartment lid opens.

Rear Compartment Lid Release Inoperative

2 |

1. Set the valet switch to the UNLOCK position.
2. Press the rear compartment lid release button on the keyless entry transmitter.

The rear compartment lid opens.

Rear Release Inoperative with Transmitter

in Keyless Entry.

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.