For 1990-2009 cars

## Radio Front Speaker Replacement Buick with UQ8

### Removal Procedure

1. Remove the IP upper trim pad. Refer Instrument Panel Upper Trim Pad Replacement in Instrument Panel, Gauges and Console.
2. Remove the fasteners.
3. Raise the speaker (1).
4. Disconnect the electrical connector(s).

### Installation Procedure

1. Connect the electrical connector(s).
2. Install the speaker (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the speaker fasteners.

Tighten
Tighten the fasteners to 1.9 N·m (17 lb in).

4. Install the IP upper trim pad. Refer Instrument Panel Upper Trim Pad Replacement in Instrument Panel, Gauges and Console.