For 1990-2009 cars

### Removal Procedure

1. Remove the trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Remove the two fasteners (2).
4. Lower the window channel (1) to the bottom of the door.
5. Remove the window channel through the opening below the door module.

### Installation Procedure

1. Install the window channel (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the fasteners (2).

Tighten
Tighten the bolts to 12 N·m (106 lb in).

3. Install the water deflector. Refer to Rear Side Door Water Deflector Replacement .
4. Install the trim panel. Refer to Rear Side Door Trim Panel Replacement .