For 1990-2009 cars

### Removal Procedure

Notice: Proper stoplamp switch adjustment is essential. Improper stoplamp switch adjustment could cause brake drag and excessive brake lining wear.

1. Remove the left sound insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.
2. Disconnect the electrical connectors.
3. Remove the release switch assembly (1).

### Installation Procedure

1. Install the release switch assembly (1).
2. Connect the electrical connectors.

Important: An incorrect adjustment may cause the cruise control system to work improperly.

3. Adjust the cruise control release switch. Refer to Cruise Release Switch Adjustment .
4. Install the left sound insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.