For 1990-2009 cars

### Removal Procedure

1. Cycle the glass panel to the rear.
2. Push out the pin (5) in the deflector left arm (1) from each side.

Important: Note the positions of the springs (3) prior to removal in order to ensure proper operation after assembly.

3. Remove the springs (3).
4. Raise the deflector left arm (1) to the vertical position.
5. Snap the molded pin (5) out of the bracket (4).

### Installation Procedure

Important: Using pliers, squeeze the bracket arms (4) in order to ensure a secure fit.

1. Install the pin (5) in the deflector arm (1) on each side.

Important: Note the position of the springs (3) to the lifter arm from the removal position.

2. Install the springs (3) to each side of the deflector arm (1).