For 1990-2009 cars

In order to provide the proper sealing and minimize the windnoise, adjust the height of the sliding glass panel in the following manner:

• |
- Equal in height from side-to-side

• |
- Front of the sliding glass panel (1), flush to 1.0 mm (0.040 in) below the roof panel (2)

• |
- Rear of the sliding glass panel, flush to 1.0 mm (0.040 in) above the roof panel

With the sliding glass panel in the closed position, inspect the height of the glass panel at the following locations:

• | The front of the glass panel

• | The rear of the glass panel

If the panel height is not within the above specifications, perform the following adjustment procedure:

Important: Adjust the sliding glass panel height one corner at a time. Only adjust the corners that are not at the proper height. After adjusting each corner, inspect the height of the entire sliding glass panel in order to determine if additional adjustment is required.

1. With the glass panel fully closed, slide the sunshade fully rearward.
2. Remove the 3 fasteners from the front edge of the shield ring. Slide the shield ring rearward.

Important: DO NOT loosen all 3 of the fasteners on the side being adjusted.

3. In order to adjust any corner, complete the following steps:

3.1. | Loosen the glass panel mounting fastener nearest to the corner being adjusted.

3.2. | Loosen the center mounting fastener on the side being adjusted.

4. After loosening the 2 fasteners, move the glass panel up or down by hand.

Tighten the 2 fasteners.

5. Inspect the sliding glass panel height.

Readjust the height as needed.

6. Repeat the adjustment procedures on the other corners as needed in order to meet the height specifications.
7. Slide the shield ring forward.
8. Install the 3 retaining fasteners.