For 1990-2009 cars

# CUPHOLDER DOES NOT STAY LATCHED

#### SUBJECT: CUPHOLDER DOES NOT STAY LATCHED (INSTALL SERVICE REPAIR KIT)

#### MODELS: 1995-98 OLDSMOBILE AURORA, EIGHTY EIGHT LS, LSS, REGENCY

#### CONDITION:

SOME CUSTOMERS MAY COMMENT THAT THE CUPHOLDER DOES NOT STAY LATCHED.

#### CORRECTION:

THE FOLLOWING PROCEDURE HAS BEEN DEVELOPED TO REPLACE THE CUP LATCH WIRE AND STRIKER (PIN ASSEMBLY) FOR CUPHOLDER DOOR CLOSURE.

#### PROCEDURE:

1. REMOVE SHIFTER TRIM PLATE. REFER TO SECTION 8C IN THE APPROPRIATE SERVICE MANUAL.

2. OBTAIN SERVICE REPLACEMENT KIT FROM GMSPO, P/N 25688508 AND FOLLOW THE INSTRUCTIONS AND ILLUSTRATIONS SUPPLIED IN THE KIT.

#### PARTS INFORMATION:

P/N DESCRIPTION ================== =============================

25688508 CUPHOLDER STRIKER SERVICE KIT

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION LABOR OPERATION NUMBER DESCRIPTION TIME =============== ========================= ==============

C2795 - AURORA PLATE, SHIFT GATE TRIM - USE PUBLISHED REPLACE LABOR OPERATION TIME

C2790 - EIGHTY PLATE, CONSOLE TRIM - USE PUBLISHED EIGHT REPLACE LABOR OPERATION TIME

ADD: LATCH REPLACEMENT 0.2 HR

FIGURES: 00

ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE

A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.