For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Fog lights System Check? | -- | Go to Step 2 | Go to Fog Lights System Check
2 | Disconnect the fog lamp switch connector. Do the fog lamps turn off? | -- | Go to Step 6 | Go to Step 3
3 | Disconnect the lamp control module (LCM) connector C2. Do the fog lamps turn off? | -- | Go to Step 7 | Go to Step 4
4 | Remove the fog lamps relay from the RH IP fuse block. Do the fog lamps turn off? | -- | Go to Step 8 | Go to Step 5
5 | Repair the short to voltage in CKT 34 (PPL). Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Fog Lights System Check | --
6 | Replace the fog lamp switch. Refer to Instrument Cluster Trim Panel Replacement . Is the repair complete? | -- | Go to Fog Lights System Check | --
7 | Replace the LCM. Is the repair complete? | -- | Go to Fog Lights System Check | --
8 | Replace the fog lamps relay. Is the repair complete? | -- | Go to Fog Lights System Check | --