For 1990-2009 cars

### Removal Procedure

1. Remove the front seats. Refer to Seat Replacement in Seats.
2. Remove the inboard seat belt buckles, as needed. Refer to Seat Belt Buckle Replacement - Left Front in Restraints.
3. Remove the seat belt retractor covers. Refer to Seat Belt Replacement - Driver in Seatbelts.
4. Remove the rear seat cushion.
5. Remove the center console, as applicable. Refer to Console Replacement in Instrument Panel, Gauges and Console.
6. Remove the lower center pillar trim.
7. Remove the carpet retainers (1).
8. Remove the finish shrouds.
9. Remove the following components from under the instrument panel:

• | The sound deadening panels

• | The insulator

• | Remove the floor carpet (2).

### Installation Procedure

1. Position the floor carpet (2).
2. Install the following components under the instrument panel:

• | The sound deadening panels

• | The insulator

3. Install the carpet retainers (1).
4. Install the lower center pillar trim.
5. Install the finish shrouds.
6. Install the center console, as applicable. Refer to Console Replacement in Instrument Panel, Gauges and Console.
7. Install the rear seat cushion.
8. Install the seat belt retractor covers. Refer to Seat Belt Replacement - Driver in Seatbelts.
9. Install the inboard seat belt buckles, as needed. Refer to Seat Belt Buckle Replacement - Left Front in Restraints.
10. Install the front seats. Refer to Seat Replacement in Seats.