For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

• | Place the headlamp switch in the OFF position.

• | Place the fog lamp switch in the OFF position.

The fog lights are off.

Fog Lamps Always On

2 |

• | Place the headlamp switch in the PARK position.

• | Place the fog lamp switch in the ON position.

The fog lights turn on.

• | Fog Lamps Inoperative - All

• | Fog Lamps Inoperative - All

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.