For 1990-2009 cars

### Removal Procedure

Caution: Disconnect the power window switch when working inside the driver door. When operated, the Express Up/Down Feature allows the door window to move very quickly, without stopping, which could cause personal injury.

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Remove the window channel fasteners.
4. Move the lower window channel (2) downward and to the front.
5. Remove the window channel (2) through the opening at the front of the door module.

### Installation Procedure

1. Install the front window channel (2).
2. Place the window channel into approximate position with the wire harness behind the channel.
3. Line up the window channel on the window and slide the window channel (2) upward in order to engage the retainer.
4. Push upward and align the lower bracket with the screw hole.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the lower bracket fastener.

Tighten
Tighten the fastener to 10 N·m (88 lb in).

6. Install the water deflector. Refer to Door Water Deflector Replacement .
7. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .