For 1990-2009 cars

### Removal Procedure

1. Remove the fuel cap.
2. Remove the screw from the latch, if equipped.
3. Remove the screws retaining the filler pipe to the filler pocket (1).
4. Remove the screws (2) retaining the filler pocket (1) to the body.
5. Remove the filler pocket (1) from the body.

### Installation Procedure

1. Install the filler pocket (1) to the body.
2. Install the screws (2) retaining the filler pocket (1) to the body.
3. Install the screws retaining the filler pipe to the filler pocket (1).
4. Install the screw to the latch, as needed.
5. Install the fuel cap.