For 1990-2009 cars

### Disassembly Procedure

#### Tools Required

J 23653-SIR Lock Plate Compressor

1. Remove the SIR coil assembly. Refer to Inflatable Restraint Steering Wheel Module Coil Disassemble - Off Vehicle
2. Remove the bearing retainer (1) using the J 23653-SIR
3. Remove the shaft lock (1).
4. Remove the turn signal cancel cam assembly (2).
5. Remove the upper bearing spring (3).
6. Remove the upper bearing inner race seat (2).

Remove the inner race (1).