For 1990-2009 cars

#### Tools Required

• | J 36850 Assembly Lubricant (or equivalent)

• | J 44538 TORX® 30+

Important: Do not use any type of adhesive or sealer when assembling the gaskets. You may use J 36850 or equivalent as an aid.

1. Install the case cover upper gasket (430) and the case cover lower gasket (429) on the case.

Important: Be careful to not move the gaskets.

2. Use J 36850 or equivalent in order to retain the fourth clutch shaft thrust washer (432) and the drive sprocket/case cover thrust washer (514) to the case cover (400).
3. Make sure that the manual valve (404) is held in place and assemble the case cover (400) onto the pins in the case.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: Do not use an impact wrench.

4. Finger start all transaxle case cover bolts (433-436) into the locations noted.

Tighten

• | Tighten the M 6 size bolts (434, 436) to 12 N·m (106 lb in).

• | Tighten the M 8 size bolts (435) to 25 N·m (18 lb ft).

• | Tighten the M 6 size bolts (433) to 12 N·m (106 lb in) using J 44538 .