For 1990-2009 cars

## Sun Load Temperature Sensor Replacement Buick

### Removal Procedure

1. Remove the defroster grille by prying up on the grille.
2. Remove the sun load sensor (1) from the defroster grille by twisting the sensor one quarter turn.
3. Disconnect the sun load sensor electrical connector.
4. Remove the sun load sensor (1).

### Installation Procedure

1. Connect the sun load sensor electrical connector.
2. Install the sun load sensor (1) to the defroster grille by twisting the sensor one quarter turn.
3. Install the defroster grille by snapping the grille into place.

## Sun Load Temperature Sensor Replacement Oldsmobile

### Removal Procedure

1. Remove the defroster grille (2) by prying up on the grille.
2. Remove the sun load sensor (1) from the defroster grille (2) by twisting the sensor one quarter turn.
3. Disconnect the sun load sensor electrical connector.
4. Remove the sun load sensor (1).

### Installation Procedure

1. Connect the sun load sensor electrical connector.
2. Install the sun load sensor (1) to the defroster grille (2) by twisting the sensor one quarter turn.
3. Install the defroster grille (2) by snapping the grille into place.

## Sun Load Temperature Sensor Replacement Pontiac

### Removal Procedure

1. Remove the defroster grille by prying up on the grille.
2. Remove the sun load sensor (1) from the defroster grille by twisting the sensor one quarter turn.
3. Disconnect the sun load sensor electrical connector.
4. Remove the sun load sensor (1).

### Installation Procedure

1. Connect the sun load sensor electrical connector.
2. Install the sun load sensor (1) to the defroster grille by twisting the sensor one quarter turn.
3. Install the defroster grille by snapping the grille into place.