For 1990-2009 cars

### Removal Procedure

1. Turn the ignition switch to the ACCY position.
2. Set the wiper switch to the PULSE position.
3. Turn the ignition off when the wipers are at the innerwipe position and not moving.
4. Remove the wiper blade from the wiper arm by pushing down on the release latch and pulling the wiper blade from the wiper arm.

### Installation Procedure

Important: Use only 22-inch beam-type blades. With the windshield wipers at the innerwipe position, the blades must be installed with the wiper blade element notches pointed toward the head casting of the wiper arm.

1. Install the wiper blade from the wiper arm.
2. Operate the wipers and check for proper operation.