For 1990-2009 cars

### Ignition Key

The ignition key for vehicles which are equipped with the PASS-Key® II system consists of the following components:

• | A typical square ignition key blank

• | A resistor pellet

The PASS-Key® II ignition key has the same mechanical key cuts as a non-PASS-Key® II ignition key. You can not service the key blank and resistor pellet separately. There are 15 different ignition key assemblies, each with a different key pellet resistance value.

When you service the PASS-Key® II system, obtain all ignition keys. Verify the proper key code values withJ 35628-A Interrogator.

### Steering Column (Ignition) Lock Cylinder

The steering column (ignition) lock cylinder that is used with the PASS-Key® II system contains a set of electrical terminals. The terminals are used to contact the resistor in the ignition key.

The wire routing for the contacts inside the steering column is very critical. When you service the lock cylinder, maintain proper wire routing.

When you replace a steering column lock cylinder, make new keys. The new keys must match the following items:

• | The PASS-Key® II code of the PASS-Key® II system

• | The mechanical cut of the new steering column (ignition) lock cylinder.