For 1990-2009 cars

#### DTC Type Table

DTC | Description | Type | Illuminate MIL
--- | --- | --- | ---
P0101 | Mass Air Flow (MAF) System Performance | A | Yes
P0102 | Mass Air Flow (MAF) Sensor Circuit Low Frequency | A | Yes
P0103 | Mass Air Flow (MAF) Sensor Circuit High Frequency | A | Yes
P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | B | Yes
P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | B | Yes
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | B | Yes
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | B | Yes
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | B | Yes
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | B | Yes
P0121 | Throttle Position (TP) Sensor Performance | A | Yes
P0122 | Throttle Position (TP) Sensor Circuit Low Voltage | A | Yes
P0123 | Throttle Position (TP) Sensor Circuit High Voltage | A | Yes
P0125 | (Engine Coolant Temperature (ECT) Excessive Time to Closed Loop | B | Yes
P0131 | Heated Oxygen Sensor (HO2S) Circuit Low Voltage Sensor 1 | B | Yes
P0132 | Heated Oxygen Sensor (HO2S) Circuit High Voltage Sensor 1 | B | Yes
P0133 | Heated Oxygen Sensor (HO2S) Circuit Slow Response Sensor 1 | B | Yes
P0134 | Heated Oxygen Sensor (HO2S) CKT Insufficient Activity Sensor 1 | B | Yes
P0135 | Heated Oxygen Sensor (HO2S) Heater Circuit Sensor 1 | B | Yes
P0137 | Heated Oxygen Sensor (HO2S) Circuit Low Voltage Sensor 2 | B | Yes
P0138 | Heated Oxygen Sensor (HO2S) Circuit High Voltage Sensor 2 | B | Yes
P0140 | Heated Oxygen Sensor (HO2S) CKT Insufficient Activity Sensor 2 | B | Yes
P0141 | Heated Oxygen Sensor (HO2S) Heater Circuit Sensor 2 | B | Yes
P0171 | Fuel Trim System Lean | B | Yes
P0172 | Fuel Trim System Rich | B | Yes
P0201 | Injector 1 Control Circuit | B | Yes
P0202 | Injector 2 Control Circuit | B | Yes
P0203 | Injector 3 Control Circuit | B | Yes
P0204 | Injector 4 Control Circuit | B | Yes
P0205 | Injector 5 Control Circuit | B | Yes
P0206 | Injector 6 Control Circuit | B | Yes
P0218 | Transmission Fluid Overtemperature | D | No
P0230 | Fuel Pump Control Circuit | D | No
P0300 | Engine Misfire Detected | B | Yes
P0325 | Knock Sensor (KS) System | D | Yes
P0327 | Knock Sensor (KS) 1 Circuit | D | No
P0332 | Knock Sensor (KS) 2 Circuit | D | No
P0336 | 18X Reference Signal Circuit | B | Yes
P0341 | Camshaft Position Sensor (CMP) Sensor Circuit Performance | B | Yes
P0401 | Exhaust Gas Recirculation (EGR) System Flow Insufficient | A | Yes
P0403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | B | Yes
P0404 | Exhaust Gas Recirculation (EGR) System Performance | B | Yes
P0405 | Exhaust Gas Recirculation (EGR) Sensor Circuit Low Voltage | B | Yes
P0420 | Three Way Catalyst (TWC) System Low Efficiency | A | Yes
P0440 | EVAP System | A | Yes
P0442 | EVAP Control System Small Leak Detected | A | Yes
P0446 | EVAP Canister Vent Blocked | A | Yes
P0452 | Fuel Tank Pressure Sensor Low Voltage | B | Yes
P0453 | Fuel Tank Pressure Sensor High Voltage | B | Yes
P0502 | Vehicle Speed Sensor (VSS) Circuit - Low Input. Refer to DTC P0502 Vehicle Speed Sensor (VSS) Circuit Low Input in Automatic Transaxle-4T65-E. | B | Yes
P0503 | Vehicle Speed Sensor (VSS) Circuit - Intermittent. Refer to DTC P0503 Vehicle Speed Sensor (VSS) Circuit Intermittent in Automatic Transaxle-4T65-E. | B | Yes
P0506 | Idle Control System Low RPM | B | Yes
P0507 | Idle Control System High RPM | B | Yes
P0530 | A/C Refrigerant Pressure Sensor Circuit | D | No
P0560 | System Voltage | D | No
P0601 | PCM Memory | B | Yes
P0602 | PCM Not Programmed | B | Yes
P0705 | Trans Range Switch Circuit | D | No
P0706 | Trans Range Switch Performance | D | No
P0711 | Transmission Fluid Temperature (TFT) Sensor Circuit Range/Performance. Refer to DTC P0711 TFT Sensor Circuit Range/Performance in Automatic Transaxle-4T65-E. | D | No
P0712 | Transmission Temperature (TFT) Sensor Circuit - Low Signal. Refer to DTC P0712 Transmission Fluid Temperature (TFT) Sensor Circuit Low Input in Automatic Transaxle-4T65-E. | D | No
P0713 | Transmission Fluid Temperature (TFT) Sensor Circuit - High Input. Refer to DTC P0713 Transmission Fluid Temperature (TFT) Sensor Circuit High Input in Automatic Transaxle-4T65-E. | D | No
P0716 | Input Speed Sensor Circuit - Intermittent. Refer to DTC P0716 Input Speed Sensor Circuit Intermittent in Automatic Transaxle-4T65-E. | B | Yes
P0717 | Input Speed Sensor Circuit - Low Input. Refer to DTC P0717 Input Speed Sensor Circuit Low Input in Automatic Transaxle-4T65-E. | B | Yes
P0719 | Brake Switch Circuit - Low Input. Refer to DTC P0719 Brake Switch Circuit Low Input in Automatic Transaxle-4T65-E. | D | No
P0724 | Brake Switch Circuit - High Input. Refer to DTC P0724 Brake Switch Circuit High Input in Automatic Transaxle-4T65-E. | D | No
P0730 | Incorrect Gear Ratio. Refer to DTC P0730 Incorrect Gear Ratio in Automatic Transaxle-4T65-E. | D | No
P0741 | Torque Converter Clutch System Stuck Off. Refer to DTC P0741 TCC System Stuck Off in Automatic Transaxle-4T65-E. | B | Yes
P0742 | Torque Converter Clutch System - Stuck On. Refer to DTC P0742 TCC System Stuck On in Automatic Transaxle-4T65-E. | A | Yes
P0748 | Pressure Control Solenoid Circuit - Electrical. Refer to DTC P0748 Pressure Control Solenoid Circuit Electrical in Automatic Transaxle-4T65-E. | D | Yes
P0751 | 1 - 2 Shift Solenoid Valve - Performance. Refer to DTC P0751 1-2 Shift Solenoid Valve Performance in Automatic Transaxle-4T65-E. | B | Yes
P0753 | 1 - 2 Shift Solenoid Control Circuit - Electrical. DTC P0753 1-2 Shift Solenoid Circuit Electrical in Automatic Transaxle-4T65-E. | A | Yes
P0756 | 2 - 3 Shift Solenoid Valve - Performance. Refer to DTC P0756 2-3 Shift Solenoid Valve Performance in Automatic Transaxle-4T65-E. | A | Yes
P0758 | 2 - 3 Shift Solenoid Circuit Electrical. Refer to DTC P0758 2-3 Shift Solenoid Circuit Electrical in Automatic Transaxle-4T65-E. | A | Yes
P1106 | Manifold Absolute Pressure (MAP) Sensor CKT Intermittent High Voltage | D | No
P1107 | Manifold Absolute Pressure (MAP) Sensor CKT Intermittent Low Voltage | D | No
P1111 | Intake Air Temperature (IAT) Sensor CKT Intermittent High Voltage | D | No
P1112 | Intake Air Temperature (IAT) Sensor CKT Intermittent Low Voltage | D | No
P1114 | Engine Coolant Temperature (ECT) Sensor CKT Intermittent Low Voltage | D | No
P1115 | Engine Coolant Temperature (ECT) Sensor CKT Intermittent High Voltage | D | No
P1121 | Throttle Position (TP) Sensor CKT Intermittent High Voltage | D | No
P1122 | Throttle Position (TP) Sensor CKT Intermittent Low Voltage | D | No
P1133 | Heated Oxygen Sensor (HO2S) Insufficient Switching Sensor 1 | B | Yes
P1134 | Heated Oxygen Sensor (HO2S) Transition Time Ratio Sensor 1 | B | Yes
P1257 | Supercharger System Overboost | D | No
P1336 | Crankshaft Position (CKP) System Variation Not Learned | A | Yes
P1351 | IC Circuit Open | B | Yes
1352 | Bypass Circuit Open | B | Yes
P1361 | IC Circuit Not Toggling | B | Yes
P1362 | Bypass Circuit Shorted | B | Yes
P1374 | 3X Reference Circuit | B | Yes
P1380 | EBCM DTC Rough Data Unusable | D | No
P1381 | Misfire Detected No EBCM/PCM Serial Data | D | No
P1404 | Exhaust Gas Recirculation (EGR) Valve Stuck Open | B | Yes
P1441 | EVAP System Flow During Non-Purge | B | Yes
P1520 | Park/Neutral (PNP) Switch Circuit | D | No
P1554 | Cruise Control Status Circuit | D | No
P1571 | TSC Desired Torque Circuit | D | No
P1573 | PCM/EBTCM Serial Data Circuit | D | No
P1619 | Engine Oil Life Monitor Reset Circuit | D | No
P1626 | Theft Deterrent System Fuel Enable CKT | D | No
P1629 | Theft Deterrent Crank Signal Malfunction | D | No
P1635 | 5 Volt Reference (A) Circuit | B | Yes
P1639 | 5 Volt Reference (B) Circuit | B | Yes
P1641 | A/C Relay Control Circuit | D | No
P1646 | Boost Control Solenoid Control Circuit | D | No
P1651 | Fan 1 Relay Control Circuit | B | Yes
P1652 | Fan 2 Relay Control Circuit | B | Yes
P1662 | Cruise Control Inhibit Control Circuit | D | No
P1665 | EVAP Vent Valve Solenoid Control Circuit
P1667 | Fuel Pump PWM Control Circuit | D | No
P1671 | MIL Control Circuit | D | No
P1672 | Low Engine Oil Level Lamp Control CKT | D | No
P1676 | EVAP Canister Purge Solenoid Control CKT | B | Yes
P1810 | Transmission Fluid Pressure Manual Valve Position Switch Assembly Circuit Malfunction. Refer to DTC P1810 TFP Valve Position Switch Circuit in Automatic Transaxle-4T65-E. | B | Yes
P1811 | Maximum Adapt and Long Shift. Refer to DTC P1811 Maximum Adapt and Long Shift in Automatic Transaxle-4T65-E. | D | No
P1860 | Torque Converter Clutch Pulse Width Modulation Solenoid Circuit - Electrical Solenoid Circuit. Refer to DTC P1860 TCC PWM Solenoid Circuit Electrical in Automatic Transaxle-4T65-E. | A | Yes
P1887 | Torque Converter Clutch Release Switch Circuit Malfunction. Refer to DTC P1887 TCC Release Switch Circuit in Automatic Transaxle-4T65-E. | B | Yes