For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: The blower motor runs with the ignition key OFF.
1 |

1. Ignition OFF.
2. Blower speed OFF.

Is the blower motor running?

--

Go to Step 2

System OK

2 | Inspect CKT 65 (PPL) for a short to voltage. Is there a short present? | -- | Go to Step 4 | Go to Step 3
3 | Replace the Blower control module. Refer to Blower Motor Control Module Replacement . Is the repair complete? | -- | System OK | --
4 | Repair the short in CKT 65 (PPL). Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | System OK | --