For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 39384-3 Torque Rod Retaining Pin

• | J 39384-10 Torque Rod Retaining Pin

1. Remove the rear compartment lid. Refer to Rear Compartment Lid Replacement .
2. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
3. Remove the rear seatback. Refer to Rear Seat Back Replacement .
4. Remove the trim panel between the rear seat and the rear window.
5. Remove the noise control sealer on the trim panel that connects the rear seat to the rear window. This will expose the bolts holding the hinge (1) to the body.
6. Complete the following steps in order to relieve the tension on the torque rods (2):

6.1. | Insert the J 39384-3 into the hinge.

6.2. | Insert the J 39384-10 over the end of the torque rod.

7. Remove the torque rod from the adjusting notches.
8. From inside the vehicle, remove the 2 bolts retaining the hinge to the body.
9. Remove the hinge (1).

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the hinge (1) to the body by installing the 2 bolts through the rear seat to the rear window panel. Have an assistant hold the hinge to the body.

Tighten
Tighten the hinge bolts to 18 N·m (13 lb ft).

Important: Properly seat the torque rod in the hinge between the rear shelf and the hinge assembly.

2. Install the torque rods (2).
3. Install the rear compartment lid.
4. Adjust the rear compartment lid as needed. Refer to Rear Compartment Lid Adjustment .
5. Install the noise control material.
6. Install the trim panel between the rear seat and the rear window.
7. Install the rear seatback. Refer to Rear Seat Back Replacement .
8. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .
9. Install the rear compartment lid. Refer to Rear Compartment Lid Replacement .