For 1990-2009 cars

1. Remove the turn signal switch assembly. Refer to Turn Signal and Multifunction Switch Assembly - Disassemble - Off Vehicle .
2. Remove the buzzer switch assembly (3).
3. Remove the lock retaining screw (2).
4. Remove the retaining clip (4) with the steering column passkey lock cylinder set terminal connector (5)
5. Remove the steering column passkey lock cyclinder set (1).
6. Disconnect and pull the steering column pass key lock cylinder set terminal connectors through the column.