For 1990-2009 cars

Condition | Cause
--- | ---
The lock system does not lock. |

• | A broken lock bolt spring

• | A worn lock bolt spring

• | A damaged sector

• | A damaged lock cylinder

• | A burr on the lock bolt

• | A damaged housing

• | A damaged rack

• | Interference between the bowl and the rack coupling

• | A binding ignition switch

• | A restricted actuator rod

• | The sector is installed incorrectly.

• | The shift lever is not in the PARK position.

• | The park lock cable is incorrectly adjusted.

• | The park lock components are damaged.