For 1990-2009 cars

### Removal Procedure

1. Remove the case side cover. Refer to Control Valve Body Cover Replacement
2. Disconnect the transaxle wiring harness.
3. Remove the pressure control solenoid (322).

### Installation Procedure

1. Install the pressure control solenoid (322).
2. Connect the transaxle wiring harness.
3. Install the case side cover. Refer to Control Valve Body Cover Replacement