For 1990-2009 cars

DTC | Description | Type | Illuminate AIR BAG Warning Lamp
--- | --- | --- | ---
B1015 | Passenger Deployment Loop Resistance High | SDM | Yes
B1016 | Passenger Deployment Loop Resistance Low | SDM | Yes
B1017 | Passenger Deployment Loop Open | SDM | Yes
B1018 | Passenger Deployment Loop Short to Ground | SDM | Yes
B1019 | Passenger Deployment Loop Short to Voltage | SDM | Yes
B1021 | Driver Deployment Loop Resistance High | SDM | Yes
B1022 | Driver Deployment Loop Resistance Low | SDM | Yes
B1024 | Driver Deployment Loop Short to Ground | SDM | Yes
B1025 | Driver Deployment Loop Short to Voltage | SDM | Yes
B1026 | Driver Deployment Loop Open | SDM | Yes
B1035 | Discriminating Sensor Circuit Closed or Short to Ground | SDM | Yes
B1036 | Discriminating Sensor Circuit Open or Short to Voltage | SDM | Yes
B1051 | Deployment Commanded | SDM | Yes
B1053 | Deployment Commanded with Loop Malfunction | SDM | Yes
B1061 | SIR Warning Lamp Malfunction | SDM | Yes
B1071 | Internal SDM Malfunction | SDM | Yes