For 1990-2009 cars

### Removal Procedure

1. Remove the push-pin from the center support (1).
2. Remove the fasteners (2) from the socket side sunshade.
3. Attach the sunshade to the center support (1).
4. Pull down on the sunshade in order to remove the sunshade from the headliner.
5. Partially lower the headliner in order to disconnect the wiring harness connector (if the vehicle is equipped with a lighted vanity mirror). Refer to Headlining Trim Panel Replacement .

### Installation Procedure

1. Connect the wiring harness connector.
2. Install the sunshade through the openings in the headliner.
3. Snap the retainer behind the headliner into place.
4. Install the fasteners (2).
5. Install the push-pins.