For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Interior Lights System Check? | -- | Go to Step 2 | Go to Interior Lamps System Check
2 |

1. Disconnect the IP compartment lamp switch connector.
2. Connect a fused jumper from the IP compartment lamp switch connector cavity B (DK BLU/WHT) to ground.

Does the IP compartment lamp turn on?

--

Go to Step 3

Go to Step 6

3 | Inspect CKT 1250 (BLK) for an open. Refer to Testing for Continuity in Wiring Systems. Was an open found? | -- | Go to Step 4 | Go to Step 5
4 | Repair the open in CKT 1250 (BLK). Refer to Wiring Repairs in Wiring Systems. Is the circuit repair complete? | -- | Go to Interior Lamps System Check | --
5 | Replace the IP compartment lamp switch. Is the IP compartment lamp switch replacement complete? | -- | Go to Interior Lamps System Check | --
6 | Inspect CKT 1732 (ORN) for an open between S254 and the IP compartment lamp. Refer to Testing for Continuity in Wiring Systems. Was an open found? | -- | Go to Step 7 | Go to Step 8
7 | Repair the open in CKT 1732 (ORN). Refer to Wiring Repairs in Wiring Systems. Is the circuit repair complete? | -- | Go to Interior Lamps System Check | --
8 | Inspect CKT 148 (DK BLU/WHT) for an open. Refer to Testing for Continuity in Wiring Systems. Was an open found? | -- | Go to Step 9 | Go to Step 10
9 | Repair the open in CKT 148 (DK BLU/WHT). Refer to Wiring Repairs in Wiring Systems. Is the circuit repair complete? | -- | Go to Interior Lamps System Check | --
10 | Replace the IP compartment lamp. Refer to Instrument Panel Compartment Lamp Replacement in Instrument Panel, Gauges and Console. Is the IP compartment lamp replacement complete? | -- | Go to Interior Lamps System Check | --