For 1990-2009 cars

The blower consists of the following components:

• | A permanent magnet type motor

• | A squirrel cage type fan

The blower operates at various speeds. The heater and A/C programmer determine the operation speeds.

The blower motor cools by having a small portion of the blower output air recirculate through the motor housing through a rubber tube.

The blower is located at the right side of the blower module (3), near the right of the vehicle.