For 1990-2009 cars

### Removal Procedure

1. Disconnect the 14-way connector from the ignition control module.
2. Disconnect the spark plug wires from the coil assemblies.
3. Remove 6 screws (1) securing the coil assemblies to the ignition control module.
4. Remove the coils (2) from the ignition control module (3).
5. Remove the ignition control module.

### Installation Procedure

1. Attach the coils to the ignition control module. Refer to Ignition Control Module Replacement .
2. Install 6 ignition coil attaching screws

Tighten:
Tighten the screws to 4-5 N·m (40 lb in).

3. Install the nuts and washers securing the ignition control module assembly to the mounting bracket.

Tighten:
Tighten the nuts to 8 N·m (70 lb in).

4. Connect the spark plug wires.
5. Connect the 14-way connector to module.