For 1990-2009 cars

## Power Seat Does Not Tilt Forward LH AG1

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Seats System Check? | -- | Go to Step 2 | Go to Power Seats System Check
2 |

1. Turn the ignition switch to the OFF position.
2. Backprobe the LH seat switch connector with a DMM from cavity K (Oldsmobile) or G (Buick/Pontiac) to ground.
3. Move the front vertical switch up.

Is the voltage within the specified range?

10-15 V

Go to Step 4

Go to Step 3

3 | Replace the LH seat switch. Refer to Power Seat Switch Replacement . Is the repair complete? | -- | Go to Power Seats System Check | --
4 |

1. Backprobe the LH seat switch connector with a DMM from cavity J (Oldsmobile), F (Buick) or H (Pontiac) to ground.
2. Move the front vertical switch down.

Is the voltage within the specified range?

10-15 V

Go to Step 5

Go to Step 3

5 |

1. Backprobe the LH seat front vertical motor with a DMM from cavity B (DK GRN) to ground.
2. Move the front vertical switch up.

Is the voltage within the specified range?

10-15 V

Go to Step 6

Go to Step 8

6 |

1. Backprobe the LH seat front vertical motor with a DMM from cavity A (DK BLU) to ground.
2. Move the front vertical switch down.

Is the voltage within the specified range?

10-15 V

Go to Step 7

Go to Step 9

7 | Replace the LH seat front vertical motor. Refer to Front Seat Adjuster Motor Replacement . Is the repair complete? | -- | Go to Power Seats System Check | --
8 | Repair the open in CKT 286 (DK GRN) between the LH seat switch and the LH seat front vertical motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Seats System Check | --
9 | Repair the open in CKT 287 (DK BLU) between the LH seat switch and the LH seat front vertical motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Seats System Check | --

## Power Seat Does Not Tilt Forward RH AG2

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Seats System Check? | -- | Go to Step 2 | Go to Power Seats System Check
2 |

1. Turn the ignition switch to the OFF position.
2. Backprobe the RH seat switch connector with a DMM from cavity R (Oldsmobile), F (Buick), or A (Pontiac) to ground.
3. Move the front vertical switch up.

Is the voltage within the specified range?

10-15 V

Go to Step 4

Go to Step 3

3 | Replace the RH seat switch. Refer to Power Seat Switch Replacement . Is the repair complete? | -- | Go to Power Seats System Check | --
4 |

1. Backprobe the RH seat switch connector with a DMM from cavity S (Oldsmobile), G (Buick) or B (Pontiac) to ground.
2. Move the front vertical switch down.

Is the voltage within the specified range?

10-15 V

Go to Step 5

Go to Step 3

5 |

1. Backprobe the RH seat front vertical motor with a DMM from cavity B (DK GRN) to ground.
2. Move the front vertical switch up.

Is the voltage within the specified range?

10-15 V

Go to Step 6

Go to Step 8

6 |

1. Backprobe the RH seat front vertical motor with a DMM from cavity A (DK BLU) to ground.
2. Move the front vertical switch down.

Is the voltage within the specified range?

10-15 V

Go to Step 7

Go to Step 9

7 | Replace the RH seat front vertical motor. Refer to Front Seat Adjuster Motor Replacement . Is the repair complete? | -- | Go to Power Seats System Check | --
8 | Repair the open in CKT 297 (DK GRN) between the RH seat switch and the RH seat front vertical motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Seats System Check | --
9 | Repair the open in CKT 298 (DK BLU) between the RH seat switch and the RH seat front vertical motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Seats System Check | --

## Power Seat Does Not Tilt Forward Pontaic w/AL7

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Seats System Check? | -- | Go to Step 2 | Go to Power Seats System Check
2 |

1. Disconnect the seat control module connector C2.
2. Briefly connect a fused jumper from the seat control module connector C2 cavity A (DK GRN) to ground.

Does the rear of the seat tilt up with the fused jumper connected?

--

Go to Step 9

Go to Step 3

3 | Briefly connect a fused jumper from the seat control module connector C2 cavity B (DK BLU) to ground. Does the rear of the seat tilt down with the fused jumper connected? | -- | Go to Step 10 | Go to Step 4
4 |

1. Reconnect the seat control module connector C2.
2. Disconnect the seat control module LH connector C3 or RH connector C4.
3. Connect a DMM from the seat control module LH connector C3 or the RH connector C4 cavity A (DK BLU) to ground.
4. Move the front vertical switch up.

Is the voltage within the specified range?

10-15 V

Go to Step 6

Go to Step 5

5 | Replace the seat control module. Is the repair complete? | -- | Go to Power Seats System Check | --
6 | Inspect for an open in the LH CKT 287 (DK BLU) or the RH CKT 298 (DK BLU) between the seat control module and the seat front vertical motor. Refer to Testing for Continuity in Wiring Systems. Is CKT 287 or CKT 298 OK? | -- | Go to Step 7 | Go to Step 12
7 | Inspect for an open in the LH CKT 1246 (DK GRN) or the RH CKT 1247 (DK GRN) between the seat front vertical motor and S363. Refer to Testing for Continuity in Wiring Systems. Is CKT 1246 or CKT 1247 OK? | -- | Go to Step 8 | Go to Step 12
8 | Replace the seat front vertical motor. Refer to Front Seat Adjuster Motor Replacement . Is the repair complete? | -- | Go to Power Seats System Check | --
9 | Inspect for an open in CKT 1518 (DK GRN) between the seat control module and the console seat switch. Refer to Testing for Continuity in Wiring Systems. Is CKT 1518 OK? | -- | Go to Step 11 | Go to Step 12
10 | Inspect for an open in CKT 1520 (DK BLU) between the seat control module and the console seat switch. Refer to Testing for Continuity in Wiring Systems. Is CKT 1520 OK? | -- | Go to Step 11 | Go to Step 12
11 | Replace the console seat switch. Is the repair complete? | -- | Go to Power Seats System Check | --
12 | Repair the suspect wiring. Refer to Wiring Repairs in Wiring Repairs. Is the repair complete? | -- | Go to Power Seats System Check | --