For 1990-2009 cars

Table 1: | C100
Table 2: | C101
Table 3: | C107
Table 4: | C108
Table 5: | C120
Table 6: | C121
Table 7: | C122
Table 8: | C123
Table 9: | C200
Table 10: | C202
Table 11: | C205
Table 12: | C206 (Buick)
Table 13: | C206 (Oldsmobile with D55)
Table 14: | C206 (Oldsmobile without D55)
Table 15: | C207 (Oldsmobile)
Table 16: | C209
Table 17: | C212 (Pontiac, Oldsmobile)
Table 18: | C301
Table 19: | C302
Table 20: | C304
Table 21: | C312
Table 22: | C324 (Buick/Oldsmobile)
Table 23: | C326
Table 24: | C341
Table 25: | C345
Table 26: | C350
Table 27: | C353
Table 28: | C400, C402
Table 29: | C401 (Oldsmobile)
Table 30: | C401 (Pontiac)
Table 31: | C406 (Pontiac)
Table 32: | C410, C411
Table 33: | C415
Table 34: | C430, C431
Table 35: | C440
Table 36: | C501, C801 (Pontiac)
Table 37: | C501, C801 (Buick/Oldsmobile)
Table 38: | C502
Table 39: | C601 (Oldsmobile, Buick)
Table 40: | C601 (Pontiac)
Table 41: | C602 (Pontiac) & C503
Table 42: | C603
Table 43: | C701
Table 44: | C702
Table 45: | C703, C803
Table 46: | C802

#### C100

Connector Part Information |

• | 12160280

• | 20 Way F Micro-Pack 100 Series (GRY)

Connector Part Information

• | 12160542

• | 20 Way M Micro-Pack 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 1222 | Shift A Solenoid Output | A | LT GRN | 1222 | Shift A Solenoid Output
B | YEL/BLK | 1223 | Shift B Solenoid Output | B | YEL/BLK | 1223 | Shift B Solenoid Output
C | RED/BLK | 1228 | Transmission Force Motor Feed | C | RED/BLK | 1228 | Transmission Force Motor Feed
D | LT BLU/WHT | 1229 | Transmission Force Motor Return | D | LT BLU/WHT | 1229 | Transmission Force Motor Return
E | PNK | 339 | Fused Output - IGN | E | PNK | 339 | Fused Output - IGN
F-K | -- | -- | Not Used | F-K | -- | -- | Not Used
L | YEL/BLK | 1227 | Transmission Temp Sensor Signal | L | YEL/BLK | 1227 | Transmission Temp Sensor Signal
M | BLK | 808 | Sensor Return | M | BLK | 808 | Sensor Return
N | PNK | 1224 | Transmission Pressure Switch Signal - Bit 1 | N | PNK | 1224 | Transmission Pressure Switch Signal - Bit 1
P | RED | 1226 | Transmission Pressure Switch Signal - Bit 3 | P | RED | 1226 | Transmission Pressure Switch Signal - Bit 3
R | DK BLU | 1225 | Transmission Pressure Switch Signal - Bit 2 | R | DK BLU | 1225 | Transmission Pressure Switch Signal - Bit 2
S | RED/BLK | 1230 | Transmission Input Speed Sensor Signal | S | RED/BLK | 1230 | Transmission Input Speed Sensor Signal
T | TAN/BLK | 418 | TCC Solenoid Output | T | TAN/BLK | 418 | TCC Solenoid Output
U | PNK | 657 | TCC Oil Pressure Switch Signal | U | PNK | 657 | TCC Oil Pressure Switch Signal
V | DK BLU/WHT | 1231 | Transmission Input Speed Sensor Return | V | DK BLU/WHT | 1231 | Transmission Input Speed Sensor Return

#### C101

Connector Part Information |

• | 12146935

• | 66 Way Metri-Pack Mixed (BLK)

Connector Part Information

• | 12129791

• | 66 Way Metri-Pack Mixed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | BLK/WHT | 251 | Ground | A1 | BLK/WHT | 251 | Ground
A2 | PNK | 439 | Fused Output-IGN | A2 | PNK | 439 | Fused Output -IGN
A3 | PNK | 339 | TCC/TRNS Fused Ignition | A3 | PNK | 339 | TCC/TRNS Fused Ignition
A4 | TAN | 31 | Oil Pressure Indicator Lamp Output | A4 | TAN | 31 | Oil Pressure Indicator Lamp Output
A5 | BRN | 437 | Vehicle Speed Sensor | A5 | -- | -- | Not Used
A6 | WHT | 1310 | Canister Vent Valve Solenoid | A6 | WHT | 1310 | Canister Vent Valve Solenoid
A7 | TAN/BLK | 464 | Traction Control System Signal -Torque Delivered | A7 | TAN/BLK | 464 | Traction Control System Signal - Torque Delivered
B1 | BLK | 1450 | Ground | B1 | BLK | 1450 | Ground
B2 | DK GRN | 59 | Air Conditioning Compressor Clutch Solenoid Feed | B2 | DK GRN | 59 | Air Conditioning Compressor Clutch Solenoid Feed
B3 | LT GRN | 36 | Coolant Temperature Signal | B3 | LT GRN | 36 | Coolant Temperature Signal
B4 | BLK | 808 | Sensor Return | B4 | BLK | 808 | Sensor Return
B5 | PNK | 639 | Fused Output -IGN | B5 | PNK | 639 | Fused Output -IGN
B6 | DK GRN/WHT | 817 | Vehicle Speed Sensor | B6 | DK GRN/WHT | 817 | Vehicle Speed Sensor
B7 | DK BLU | 229 | Vehicle Anti-Theft System Signal -Disable Engine | B7 | DK BLU | 229 | Vehicle Anti-Theft System Signal - Disable Engine
C2 | TAN | 800 | UART Serial Data Signal | C2 | TAN | 800 | UART Serial Data Signal
C3 | PNK/BLK | 1379 | Oil Change Reset Signal | C3 | PNK/BLK | 1379 | Oil Change Reset Signal (w/L67)
C4 | WHT | 776 | Transmission Position Switch Signal-Parity Bit | C4 | WHT | 776 | Transmission Position Switch Signal-Parity Bit
C5 | PPL | 1589 | Fuel Gauge Sensor Signal | C5 | PPL | 1589 | Fuel Gauge Sensor Signal
C7 | PPL | 1490 | CCR Module Signal-Wide Open Throttle | C7 | PPL | 1490 | CCR Module Signal-Wide Open Throttle
D1 | PNK | 839 | Fused Output -IGN | D1 | PNK | 839 | Fused Output-IGN
D2 | PNK | 239 | Fused Output - IGN | D2 | PNK | 239 | Fused Output - IGN (w/L36)
D3 | PPL | 1807 | Class 2 Serial Data Line | D3 | PPL | 1807 | Class 2 Serial Data Line
D4 | PPL | 420 | Brake Pedal Switch Output -Torque Converter Clutch | D4 | PPL | 420 | Brake Pedal Switch Output -Torque Converter Clutch
D5 | DK GRN/WHT | 459 | Air Conditioning Compressor Control Relay Output -Coil | D5 | DK GRN/WHT | 459 | Air Conditioning Compressor Control Relay Output -Coil
D6 | GRY | 705 | Reference Voltage Feed | D6 | -- | -- | Not Used
D7 | PPL/WHT | 455 | Fuel Level PWM Output Signal From PCM | D7 | PPL/WHT | 455 | Fuel Level PWM Output Signal From PCM
E7 | DK GRN/WHT | 762 | Air Conditioning Request Signal W-CJZ, C68 | E7 | DK GRN/WHT | 762 | Air Conditioning Request Signal W-CJZ, C68
F1 | PPL | 6 | Starter Solenoid Feed | F1 | PPL | 6 | Starter Solenoid Feed
F7 | BLK | 891 | Boost Gage Signal | F7 | BLK | 891 | Boost Gage Signal
G2 | WHT | 345 | Variable Assist Low Effort | G2 | WHT | 345 | Variable Assist Low Effort
G6 | GRY | 1787 | Variable Assist Motor Feed High Effort | G6 | GRY | 1787 | Variable Assist Motor Feed High Effort
G7 | RED | 1642 | Fused Output -Bat | G7 | RED | 1642 | Fused Output - Bat
H1 | DK GRN | 335 | Coolant Fan Relay Output - Coil | H1 | DK GRN | 335 | Coolant Fan Relay Output - Coil
H3 | WHT | 85 | Cruise Control Indicator Lamp Output | H3 | WHT | 85 | Cruise Control Indicator Lamp Output
H4 | ORN/BLK | 463 | Traction Control System Signal -Torque Desired | H4 | ORN/BLK | 463 | Traction Control System Signal -Torque Desired
H5 | LT BLU | 553 | Trans Shift Select Switch Output -Performance | H5 | LT BLU | 553 | Trans Shift Select Switch Output -Performance (w/L36)
H7 | PNK | 1039 | Fused Output - IGN | H7 | PNK | 1039 | Fused Output - IGN
J1 | BRN | 25 | Charge Indicator Lamp Output | J1 | BRN | 25 | Charge Indicator Lamp Output
J3 | GRY | 605 | Reference Voltage Feed | J3 | GRY | 605 | Reference Voltage Feed
J4 | DK BLU | 473 | Coolant Fan Relay Output - Coil Secondary | J4 | DK BLU | 473 | Coolant Fan Relay Output - Coil Secondary
J5 | DK GRN/WHT | 465 | Fuel Pump Relay Feed - Coil | J5 | DK GRN/WHT | 465 | Fuel Pump Relay Feed - Coil
J7 | WHT | 121 | Tachometer Signal | J7 | WHT | 121 | Tachometer Signal
K1 | BRN/WHT | 419 | Check Engine Indicator Lamp Output | K1 | BRN/WHT | 419 | Check Engine Indicator Lamp Output
K2 | BLK/WHT | 771 | Transmission Position Switch Signal - Bit 1 | K2 | BLK/WHT | 771 | Transmission Position Switch Signal - Bit 1
K3 | DK GRN | 83 | Cruise Control Signal - Disengage | K3 | DK GRN | 83 | Cruise Control Signal - Disengage
K4 | BRN/WHT | 1173 | Low Oil Level Indicator Lamp Output | K4 | BRN/WHT | 1173 | Low Oil Level Indicator Lamp Output
K6 | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | K6 | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
K7 | DK GRN | 35 | Coolant Temperature Indicator Lamp Output | K7 | DK GRN | 35 | Coolant Temperature Indicator Lamp Output
L2 | BLK/WHT | 451 | Ground | L2 | BLK/WHT | 451 | Ground
L3 | YEL | 772 | Transmission Position Switch Signal - Bit 2 | L3 | YEL | 772 | Transmission Position Switch Signal - Bit 2
L4 | GRY | 773 | Transmission Position Switch Signal - Bit 3 | L4 | GRY | 773 | Transmission Position Switch Signal - Bit 3
L5 | GRY | 803 | Change Oil Indicator Lamp Output | L5 | -- | -- | Not Used
L6 | ORN/BLK | 434 | Neutral Safety Switch Signal | L6 | ORN/BLK | 434 | Neutral Safety Switch Signal

#### C107

Connector Part Information |

• | 12047937

• | 8 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047931

• | 8 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 423 | Electronic Spark Timing Control Signal | A | WHT | 423 | Electronic Spark Timing Control Signal
B | TAN/BLK | 424 | Electronic Spark Timing Bypass Signal | B | TAN/BLK | 424 | Electronic Spark Timing Bypass Signal
C | LT BLU/BLK | 647 | Crankshaft Position Signal | C | LT BLU/BLK | 647 | Crankshaft Position Signal
D | PPL/WHT | 430 | Electronic Spark Timing High Reference Signal | D | PPL/WHT | 430 | Electronic Spark Timing High Reference Signal
E | WHT | 121 | Tachometer Signal | E | WHT | 121 | Tachometer Signal
F | BLK | 630 | Camshaft Position Signal | F | BLK | 630 | Camshaft Position Signal
G | RED/BLK | 453 | Electronic Spark Timing Low Reference Signal | G | RED/BLK | 453 | Electronic Spark Timing Low Reference Signal
H | PNK | 239 | Fused Output - Ign 1 | H | PNK | 239 | Fused Output - Ign 1

#### C108

Connector Part Information |

• | 12010973

• | 2 Way F Weather Pack (BLK)

Connector Part Information

• | 12015792

• | 2 Way M Weather Pack (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT BLU | 14 | Turn Signal Lamp Feed-Left Front | A | LT BLU | 14 | Turn Signal Lamp Feed-Left Front
B | BLK | 1150 | Ground | B | LT BLU | 1150 | Ground

#### C120

Connector Part Information |

• | 12052638

• | 2 Way F Metri-Pack 150 Series (LT GRY)

Connector Part Information

• | 12162343

• | 2 Way M Metri-Pack 150 Series (LT GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 873 | Wheel Speed Sensor Return-Left Front | A | WHT | 873 | Wheel Speed Sensor Return-Left Front
B | BLK | 830 | Wheel Speed Sensor Signal-Left Front | B | BLK | 830 | Wheel Speed Sensor Signal-Left Front

#### C121

Connector Part Information |

• | 12052638

• | 2 Way F Metri-Pack 150 Series (LT GRY)

Connector Part Information

• | 12162343

• | 2 Way M Metri-Pack 150 Series (LT GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 833 | Wheel Speed Sensor Return-Right Front | A | WHT | 833 | Wheel Speed Sensor Return-Right Front
B | BLK | 872 | Wheel Speed Sensor Signal-Right Front | B | BLK | 872 | Wheel Speed Sensor Signal-Right Front

#### C122

Connector Part Information |

• | 12065861

• | 5 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12084672

• | 5 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 11 | High Beam Headlamp Feed | A | LT GRN | 11 | High Beam Headlamp Feed
B | TAN | 12 | Low Beam Headlamp Feed | B | TAN | 12 | Low Beam Headlamp Feed
C | ORN | 58 | Cornering Lamp Feed-Right (w/T87) | C | ORN | 58 | Cornering Lamp Feed-Right (w/T87)
D | -- | -- | Not Used | D | -- | -- | Not Used
E | BLK | 1550 | Ground | E | BLK | 1550 | Ground

#### C123

Connector Part Information |

• | 12084890

• | 5 Way F Metri-Pack 280 Series (GRY)

Connector Part Information

• | 12085015

• | 5 Way M Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 11 | High Beam Headlamp Feed | A | LT GRN | 11 | High Beam Headlamp Feed
B | TAN | 12 | Low Beam Headlamp Feed | B | TAN | 12 | Low Beam Headlamp Feed
C | ORN | 57 | Cornering Lamp Feed - Left w/T87 | C | ORN | 57 | Cornering Lamp Feed - Left w/T87
C | -- | -- | Not Used | C | -- | -- | Not Used
D | GRY | 589 | Daytime Running Lamp Resistor Feed | D | GRY | 589 | Daytime Running Lamp Resistor Feed
E | BLK | 1150 | Ground | E | BLK | 1150 | Ground

#### C200

Connector Part Information |

• | 12162542

• | 116 Way F Metri-Pack (BLK)

Connector Part Information

• | 12162543

• | 116 Way M Metri-Pack (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A2 | DK BLU | 15 | RH Front Turn Signal Lamp Feed | A2 | DK BLU | 15 | RH Front Turn Signal Lamp Feed
A3 | LT BLU | 1785 | Park Lamp Switch Output - Park Lamps Off | A3 | LT BLU | 1785 | Park Lamp Switch Output - Park Lamps Off
A4 | BRN | 368 | SIR Indicator Lamp Output | A4 | BRN | 358 | SIR Indicator Lamp Output
A5 | TAN | 31 | Oil Pressure Indicator Lamp Output | A5 | TAN | 31 | Oil Pressure Indicator Lamp Output
A6 | WHT | 121 | Tachometer Signal | A6 | WHT | 121 | Tachometer Signal
A7 | ORN/BLK | 434 | Neutral Safety Switch Signal | A7 | ORN/BLK | 434 | Neutral Safety Switch Signal
A8 | LT GRN | 36 | Coolant Temp Signal | A8 | LT GRN | 36 | Coolant Temp Signal
A8 | DK GRN | 135 | Coolant Temp Sensor Signal (Pontiac) | A8 | DK GRN | 135 | Coolant Temp Sensor Signal (Pontiac)
A9 | YEL | 317 | Fog Lamp Relay Feed - Coil (Oldsmobile) | A9 | YEL | 317 | Fog Lamp Relay Feed - Coil (Oldsmobile)
A9 | BLK | 891 | Boost Gage Signal (Pontiac) | A9 | BLK | 891 | Boost Gage Signal (Pontiac)
A11 | LT GRN/BLK | 875 | ABS Indicator Lamp Driver Module Output | A11 | LT GRN/BLK | 875 | ABS Indicator Lamp Driver Module Output
A12 | BRN/WHT | 1571 | Traction Control System Switch Signal | A12 | BRN/WHT | 1571 | Traction Control System Switch Signal
A13 | LT GRN | 11 | High Beam Headlamp Feed (Pontiac) | A13 | LT GRN | 11 | High Beam Headlamp Feed (Pontiac)
A13 | LT GRN/BLK | 1360 | High Beam Ind Lamp Output (Buick) | A13 | LT GRN/BLK | 1360 | High Beam Ind Lamp Output (Buick)
B1 | PNK/BLK | 1379 | Oil Change Reset Switch Signal | B1 | PNK/BLK | 1379 | Oil Change Reset Switch Signal
B2 | YEL | 32 | Fused Output - IP Lamps | B2 | YEL | 32 | Fused Output - IP Lamps
B3 | BRN/WHT | 1434 | Computer Command Ride Switch Signal - Firm | B3 | BRN/WHT | 1434 | Computer Command Ride Switch Signal - Firm
B4 | BRN | 1141 | Fused Output - Ign | B4 | BRN | 1141 | Fused Output - Ign
B5 | WHT | 17 | Stoplamp Switch Output (Buick/Oldsmobile) | B5 | WHT | 17 | Stoplamp Switch Output (Buick/Oldsmobile)
B5 | LT BLU | 20 | Stoplamp Feed (Pontiac) | B5 | LT BLU | 20 | Stoplamp Feed (Pontiac)
B6 | DK BLU | 1393 | Interior Lamp Relay Output - Coil | B6 | DK BLU | 1393 | Interior Lamp Relay Output - Coil
B7 | TAN/WHT | 33 | Brake Warning Indicator Lamp Output | B7 | TAN/WHT | 33 | Brake Warning Indicator Lamp Output
B8 | WHT | 17 | Stoplamp Switch Output (Buick/Oldsmobile) | B8 | WHT | 17 | Stoplamp Switch Output (Buick/Oldsmobile)
B8 | LT BLU | 20 | Stoplamp Feed (Pontiac) | B8 | LT BLU | 20 | Stoplamp Feed (Pontiac)
B9 | TAN | 1278 | Lamp Monitor Data Request Signal | B9 | TAN | 1278 | Lamp Monitor Data Request Signal
B10 | WHT | 1279 | Lamp Monitor Data Signal | B10 | WHT | 1279 | Lamp Monitor Data Signal
B12 | BRN/WHT | 419 | Check Engine Indicator Lamp Output | B12 | BRN/WHT | 419 | Check Engine Indicator Lamp Output
B13 | TAN | 800 | UART Serial Data Signal | B13 | TAN | 800 | UART Serial Data Signal
C1 | DK GRN | 35 | Coolant Temperature Indicator Lamp Output | C1 | DK GRN | 35 | Coolant Temperature Indicator Lamp Output
C2 | LT BLU | 14 | LH Front Turn Signal Lamp Feed | C2 | LT BLU | 14 | LH Front Turn Signal Lamp Feed
C3 | DK GRN | 145 | Power Antenna Relay Feed-Coil | C3 | DK GRN | 145 | Power Antenna Relay Feed-Coil
C4 | BRN | 25 | Charge Indicator Lamp Output | C4 | BRN | 25 | Charge Indicator Lamp Output
C5 | PNK/BLK | 109 | Hood Ajar Switch Signal | C5 | PNK/BLK | 109 | Hood Ajar Switch Signal
C6 | TAN | 800 | UART Serial Data Signal | C6 | TAN | 800 | UART Serial Data Signal
C7 | PPL | 1397 | Air Conditioning Switch Signal - Heat Solenoid Control | C7 | PPL | 1397 | Air Conditioning Switch Signal - Heat Solenoid Control
C8 | PNK | 1396 | A/C Switch Signal Defrost Solenoid Control | C8 | PNK | 1396 | A/C Switch Signal Defrost Solenoid Control
C9 | LT GRN | 1395 | A/C Switch Signal Vent Solenoid Control | C9 | LT GRN | 1395 | A/C Switch Signal Vent Solenoid Control
C10 | DK GRN | 1394 | A/C Switch Signal Air Condition Solenoid Control | C10 | DK GRN | 1394 | A/C Switch Signal Air Condition Solenoid Control
C11 | ORN | 440 | Fused Output - Bat | C11 | ORN | 440 | Fused Output - Bat
C12 | BRN | 247 | Blower Enable Relay Output-Coil | C12 | BRN | 247 | Blower Enable Relay Output-Coil
C13 | TAN | 800 | UART Serial Data Signal | C13 | TAN | 800 | UART Serial Data Signal
D1 | PNK | 439 | Fused Output - Ign | D1 | PNK | 439 | Fused Output - Ign
D2 | TAN | 800 | UART Serial Data Signal | D2 | TAN | 800 | UART Serial Data Signal
D3 | DK GRN/WHT | 817 | Vehicle Speed Signal | D3 | DK GRN/WHT | 817 | Vehicle Speed Signal
D4 | ORN | 40 | Fused Output - Bat | D4 | ORN | 40 | Fused Output - Bat
D5 | PPL | 1881 | HVAC Control Assembly Signal-Clock Timer | D5 | PPL | 1881 | HVAC Control Assembly Signal-Clock Timer
D6 | LT BLU | 1880 | HVAC Control Assembly Signal-Driver | D6 | LT BLU | 1880 | HVAC Control Assembly Signal-Driver
D10 | GRY | 910 | Reference Voltage Feed | D10 | GRY | 705 | Reference Voltage Feed
D12 | YEL | 234 | Seat Belt Indicator Lamp Output | D12 | YEL | 234 | Seat Belt Indicator Lamp Output
E1 | YEL | 10 | Headlamp Switch Output | E1 | YEL | 10 | Headlamp Switch Output
E2 | YEL | 60 | Blower Switch Output - Low (Pontiac/Oldsmobile) | E2 | YEL | 60 | Blower Switch Output - Low (Pontiac/Oldsmobile)
E2 | LT BLU | 188 | Electronic Climate Control - Blower Enable Relay Output (Buick) | E2 | LT BLU | 188 | Electronic Climate Control - Blower Enable Relay Output (Buick)
E11 | ORN | 1140 | Fused Output-Battery | E11 | ORN | 1140 | Fused Output-Battery
E12 | TAN | 63 | Blower Switch Output-Medium 1 | E12 | TAN | 63 | Blower Switch Output-Medium 1
F1 | PPL | 293 | Rear Defogger Element Feed | F1 | PPL | 293 | Rear Defogger Element Feed
F2 | PNK | 739 | Fused Output - Ign | F2 | PNK | 739 | Fused Output - Ign
F11 | ORN | 240 | Fused Output - Bat | F11 | ORN | 240 | Fused Output - Bat
F12 | BLK | 1250 | Ground | F12 | BLK | 1250 | Ground
G1 | BRN | 41 | Fused Output - Ign | G1 | BRN | 41 | Fused Output - Ign
G2 | LT BLU | 72 | Blower Switch Output-Medium 2 | G2 | LT BLU | 72 | Blower Switch Output-Medium 2
G12 | RED | 242 | Fused Output - Bat | G12 | RED | 242 | Fused Output - Bat
H1 | ORN | 1732 | Inadvertent Load Control | H1 | ORN | 1732 | Inadvertent Load Control
H3 | GRY | 8 | Instrument Panel Lamp Feed | H3 | GRY | 8 | Instrument Panel Lamp Feed
H4 | DK GRN | 1435 | Coolant Temperature Sensor Signal | H4 | DK GRN | 1435 | Coolant Temperature Sensor Signal
H5 | BLK/WHT | 251 | Ground | H5 | BLK/WHT | 251 | Ground
H6 | BLK/WHT | 1704 | Sensor Return | H6 | BLK/WHT | 1704 | Sensor Return
H7 | DK GRN | 835 | Diagnostic Signal - E and C | H7 | DK GRN | 835 | Diagnostic Signal - E and C
H8 | PPL | 1783 | Twilight Sentinel Delay Signal | H8 | PPL | 1783 | Twilight Sentinel Delay Signal
H9 | YEL/BLK | 1784 | Twilight Sentinel Enable Signal | H9 | YEL/BLK | 1784 | Twilight Sentinel Enable Signal
H10 | WHT | 278 | Photocell Signal | H10 | WHT | 278 | Photocell Signal
H11 | BLK/WHT | 451 | Ground | H11 | BLK/WHT | 451 | Ground
H12 | DK BLU | 1660 | Traction Indicator Lamp Driver Module Output | H12 | DK BLU | 1660 | Traction Indicator Lamp Driver Module Output
J1 | GRY/BLK | 745 | LH Front Door Ajar Switch Signal | J1 | GRY/BLK | 745 | LH Front Door Ajar Switch Signal
J2 | LT BLU/BLK | 747 | LH Rear Door Ajar Switch Signal | J2 | LT BLU/BLK | 747 | LH Rear Door Ajar Switch Signal
J3 | LT GRN/BLK | 748 | RH Rear Door Ajar Switch Signal | J3 | LT GRN/BLK | 748 | RH Rear Door Ajar Switch Signal
J4 | BLK | 1450 | Ground | J4 | BLK | 1450 | Ground
J6 | DK GRN | 734 | Inside Temperature Sensor Signal | J6 | DK GRN | 734 | Inside Temperature Sensor Signal
J8 | ORN | 52 | Blower Switch Output High | J8 | ORN | 52 | Blower Switch Output High
J9 | DK GRN | 264 | Security Indicator Lamp Feed | J9 | DK GRN | 264 | Security Indicator Lamp Feed
J10 | DK BLU | 85 | Cruise Control Signal - Disengage | J10 | DK BLU | 85 | Cruise Control Signal - Disengage
J11 | BRN/WHT | 1173 | Low Oil Level Indicator Lamp Output | J11 | BRN/WHT | 1173 | Low Oil Level Indicator Lamp Output
J12 | YEL | 43 | Fused Output - Acc | J12 | YEL | 43 | Fused Output - Acc
J13 | LT GRN | 1011 | Remote Radio Control Signal | J13 | LT GRN | 1011 | Remote Radio Control Signal
K1 | BLK/WHT | 746 | RH Front Door Ajar Switch Signal | K1 | BLK/WHT | 746 | RH Front Door Ajar Switch Signal
K2 | BLK/WHT | 251 | Ground | K2 | BLK/WHT | 251 | Ground
K3 | PPL/WHT | 336 | Compass Digital Signal | K3 | PPL/WHT | 336 | Compass Digital Signal
K4 | TAN/WHT | 337 | Compass Clock Signal | K4 | TAN/WHT | 337 | Compass Clock Signal
K6 | LT GRN | 66 | A/C Switch Output | K6 | LT GRN | 66 | A/C Switch Output
K7 | GRY | 1548 | Solar Sensor Signal-Passenger | K7 | GRY | 1548 | Solar Sensor Signal-Passenger
K8 | WHT | 193 | Rear Defogger Relay Output-Coil | K8 | WHT | 193 | Rear Defogger Relay Output-Coil
K9 | YEL | 1791 | Air Temperature Valve Motor Return | K9 | YEL | 1791 | Air Temperature Valve Motor Return
K10 | DK BLU | 1199 | Air Temperature Valve Motor Feed | K10 | DK BLU | 1199 | Air Temperature Valve Motor Feed
K12 | PPL/WHT | 455 | Fuel Gauge Signal | K12 | PPL/WHT | 455 | Fuel Gauge Signal
K13 | LT BLU | 553 | Transmission Select Shift Output Performance | K13 | LT BLU | 553 | Transmission Select Shift Output Performance
L1 | LT GRN | 1845 | Multi-Function Chime Control Signal | L1 | LT GRN | 1845 | Multi-Function Chime Control Signal
L2 | PNK | 1438 | CCR LED Feed Normal | L2 | PNK | 1438 | CCR LED Feed Normal
L3 | PPL/WHT | 724 | Vacuum Fluorescent Dimming Signal (Buick/Oldsmobile) | L3 | PPL/WHT | 724 | Vacuum Fluorescent Dimming Signal (Buick/Oldsmobile)
L3 | DK GRN | 1437 | CCR LED Feed - Firm (Pontiac) | L3 | DK GRN | 1437 | CCR LED Feed - Firm (Pontiac)
L4 | BRN | 9 | Park Lamp Feed | L4 | BRN | 9 | Park Lamp Feed
L5 | LT BLU | 74 | Park Lamp Switch Output | L5 | LT BLU | 74 | Park Lamp Switch Output
L5 | YEL/BLK | 68 | Low Coolant Level Indicator Lamp Output | L5 | YEL/BLK | 68 | Low Coolant Level Indicator Lamp Output
L6 | RED/BLK | 744 | Rear Compartment Ajar Switch Signal | L6 | RED/BLK | 744 | Rear Compartment Ajar Switch Signal
L7 | LT BLU/BLK | 590 | Solar Sensor Signal-Driver | L7 | LT BLU/BLK | 590 | Solar Sensor Signal-Driver
L8 | BLK | 808 | Sensor Return | L8 | BLK | 808 | Sensor Return
L10 | DK GRN/WHT | 1135 | BTSI Solenoid Feed | L10 | DK GRN/WHT | 1135 | BTSI Solenoid Feed
L11 | BLK/WHT | 99 | Windshield Washer Fluid Level Signal | L11 | BLK/WHT | 99 | Windshield Washer Fluid Level Signal
L13 | LT BLU | 1344 | Rear Compartment Release Relay Output-Coil | L13 | LT BLU | 1344 | Rear Compartment Release Relay Output-Coil

#### C202

Connector Part Information |

• | 12084183

• | 48 Way F Metri-Pack Mixed (NAT)

Connector Part Information

• | 12084133

• | 48 Way M Metri-Pack Mixed (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | YEL | 43 | Fused Output - Acc | A1 | YEL | 43 | Fused Output - Acc
A2 | GRY | 8 | Instrument Panel Lamp Feed | A2 | GRY | 8 | Instrument Panel Lamp Feed
A4 | LT GRN | 1011 | Remote Radio Control Signal | A4 | LT GRN | 1011 | Remote Radio Control Signal
A5 | WHT | 17 | Stoplamp Switch Output | A5 | WHT | 17 | Stoplamp Switch Output
A6 | DK GRN | 19 | Stoplamp Turn Lamp Feed - RH Rear | A6 | DK GRN | 19 | Stoplamp Turn Lamp Feed - RH Rear
A7 | YEL | 18 | Stoplamp, Turn Lamp Feed - LH Rear | A7 | YEL | 18 | Stoplamp, Turn Lamp Feed - LH Rear
A8 | PPL | 16 | Turn Signal Flasher Output | A8 | PPL | 16 | Turn Signal Flasher Output
A9 | BRN | 27 | Hazard Flasher Output | A9 | BRN | 27 | Hazard Flasher Output
A10 | DK BLU | 15 | Turn Signal Lamp Feed - RH Front | A10 | DK BLU | 15 | Turn Signal Lamp Feed - RH Front
A11 | LT BLU | 14 | Turn Signal Lamp Feed LH Front | A11 | LT BLU | 14 | Turn Signal Lamp Feed LH Front
-- | BLK | 28 | Horn Relay Output - Coil | A12 | BLK | 28 | Horn Relay Output - Coil
A13 | LT GRN | 80 | Key Reminder Switch Signal | A13 | LT GRN | 80 | Key Reminder Switch Signal
A14 | BLK | 1250 | Ground | A14 | BLK | 1250 | Ground
A15 | BLK | 58 | RH Cornering Lamp Feed | A15 | BLK | 58 | RH Cornering Lamp Feed
A16 | ORN | 57 | LH Cornering Lamp Feed | A16 | ORN | 57 | LH Cornering Lamp Feed
A17 | TAN | 1654 | Fused Output - Perimeter Lighting (Buick) | A17 | TAN | 1654 | Fused Output - Perimeter Lighting (Buick)
A17 | PNK | 539 | Fused Output - Ign (Oldsmobile) | A17 | PNK | 539 | Fused Output - Ign (Oldsmobile)
B2 | LT BLU | 26 | Ignition Switch Output - Off, Run | B2 | LT BLU | 26 | Ignition Switch Output - Off, Run
B3 | TAN/WHT | 33 | Brake Warning Indicator Output (Pontiac/Buick) | B3 | TAN/WHT | 33 | Brake Warning Indicator Output (Pontiac/Buick)
B3 | PPL | 209 | Brake Fluid Level Indicator Output (Oldsmobile) | B3 | PPL | 209 | Brake Fluid Level Indicator Output (Oldsmobile)
B4 | TAN | 12 | Low Beam Headlamp Feed | B4 | TAN | 12 | Low Beam Headlamp Feed
B5 | LT GRN | 11 | High Beam Headlamp Feed | B5 | LT GRN | 11 | High Beam Headlamp Feed
B5 | PPL | 524 | High Beam Headlamp Dimmer Switch Output | B5 | PPL | 524 | High Beam Headlamp Dimmer Switch Output
B6 | YEL | 5 | Ignition Switch Output - Crank | B6 | YEL | 5 | Ignition Switch Output - Crank
C2 | ORN | 300 | Ignition Switch Output - Ignition 3 | C2 | ORN | 300 | Ignition Switch Output - Ignition 3
C4 | RED | 242 | Fused Output - Bat | C4 | RED | 242 | Fused Output - Bat
C5 | BLK/WHT | 251 | Ground (Buick) | C5 | BLK/WHT | 251 | Ground (Buick)
C5 | LT BLU | 1346 | Headlamp Relay Output - N.O. Contact (Oldsmobile) | C5 | LT BLU | 1346 | Headlamp Relay Output - N.O. Contact (Oldsmobile)
C5 | YEL | 10 | Headlamp Switch Output (Pontiac) | C5 | YEL | 10 | Headlamp Switch Output (Pontiac)
D2 | RED | 1242 | Fused Output - Ign 1 | D2 | RED | 1242 | Fused Output - Ign 1
E1 | BRN | 1141 | Fused Output - Ign | E1 | BRN | 1141 | Fused Output - Ign
E2 | GRY | 397 | Cruise Control On Switch Output | E2 | GRY | 397 | Cruise Control On Switch Output
E3 | DK BLU | 84 | Cruise Control Set/Coast Switch Signal | E3 | DK BLU | 84 | Cruise Control Set/Coast Switch Signal
E4 | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal | E4 | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal
E5 | YEL | 143 | Fused Output - Acc | E5 | YEL | 143 | Fused Output - Acc
E6 | GRY | 91 | Windshield Wiper Relay Feed-Coil | E6 | GRY | 91 | Windshield Wiper Relay Feed-Coil
E7 | DK GRN | 95 | Windshield Wiper Motor Feed - Low Speed | E7 | DK GRN | 95 | Windshield Wiper Motor Feed - Low Speed
E8 | PPL | 92 | Windshield Wiper Motor Feed - High Speed | E8 | PPL | 92 | Windshield Wiper Motor Feed - High Speed
E9 | PNK | 94 | Windshield Washer Switch Signal | E9 | PNK | 94 | Windshield Washer Switch Signal
E12 | WHT/BLK | 1073 | Ignition Key Resistor Feed | E12 | WHT/BLK | 1073 | Ignition Key Resistor Feed
E13 | PPL/WHT | 1074 | Ignition Key Resistor Return | E13 | PPL/WHT | 1074 | Ignition Key Resistor Return

#### C205

Connector Part Information |

• | 12047886

• | 8 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12084256

• | 8 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 24 | Back Up Lamp Feed | A | LT GRN | 24 | Back Up Lamp Feed
B | PNK | 39 | Fused Output - Ign 1 | B | PNK | 39 | Fused Output - Ign 1
C | BLK | 1250 | Ground | C | BLK | 1250 | Ground
D | YEL | 317 | Fog Lamp Relay Feed-Coil (Pontiac) | D | YEL | 317 | Fog Lamp Relay Feed-Coil (Pontiac)
E | BRN | 9 | Park Lamp Feed (Pontiac) | E | BRN | 9 | Park Lamp Feed (Pontiac)
E | PNK | 1691 | Automatic Day/Night Mirror Return Outside (Buick/Oldsmobile) | E | PNK | 1691 | Automatic Day/Night Mirror Return Outside (Buick/Oldsmobile)
F | -- | 1732 | Not Used | -- | -- | -- | Not Used
G | WHT | 156 | Courtesy Lamp Output | G | WHT | 156 | Courtesy Lamp Output
H | BLK/WHT | 251 | Ground | H | BLK/WHT | 251 | Ground

#### C206 (Buick)

Connector Part Information |

• | 12047781

• | 3 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047782

• | 3 Way M Metri-Pack 150 Series (BLK)--

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 440 | Fuse Output - Battery | A | ORN | 440 | Fuse Output - Battery
B | BLK | 1250 | Ground | B | BLK | 1250 | Ground
C | BRN | 358 | SIR Indicator Lamp Output | C | BRN | 358 | SIR Indicator Lamp Output

#### C206 (Oldsmobile with D55)

Connector Part Information |

• | 12047781

• | 3 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047782

• | 3 Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 440 | Fuse Output - Battery | A | ORN | 440 | Fuse Output - Battery
B | BLK | 1250 | Ground | B | BLK | 1250 | Ground
C | BRN | 8 | Instrument Panel Lamp Feed | C | BRN | 8 | Instrument Panel Lamp Feed

#### C206 (Oldsmobile without D55)

Connector Part Information |

• | 12129136

• | 4 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129135

• | 4 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 440 | Fuse Output - Battery - Type III Fuse | A | ORN | 440 | Fuse Output - Battery - Type III Fuse
B | BLK | 1250 | Ground | B | BLK | 1250 | Ground
C | GRY | 8 | Instrument Panel Lamp Feed | C | GRY | 8 | Instrument Panel Lamp Feed
D | PNK | 739 | Fuse Output - Ignition 1 - Type III Fuse | D | PNK | 739 | Fuse Output - Ignition 1 - Type III Fuse

#### C207 (Oldsmobile)

Connector Part Information |

• | 12064762

• | 6 Way F Metri-Pack 150 Series (GRY)

Connector Part Information

• | 12064763

• | 6 Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 200 | Speaker Feed - Right Front | A | TAN | 200J | Speaker Feed - Right Front
B | DK GRN | 117 | Speaker Return - Right Front | B | DK GRN | 117J | Speaker Return - Right Front
C | DK BLU | 46 | Speaker Feed - Right Rear | C | DK BLU | 46F | Speaker Feed - Right Rear
D | LT BLU | 115 | Speaker Return - Right Rear | D | LT BLU | 115F | Speaker Return - Right Rear
E | BRN | 199 | Speaker Feed - Left Rear | E | BRN | 199F | Speaker Feed - Left Rear
F | YEL | 116 | Speaker Return - Left Rear | F | YEL | 116F | Speaker Return - Left Rear

#### C209

Connector Part Information |

• | 12047785

• | 4 Way F Metri-Pack 150 (BLK)

Connector Part Information

• | 12065182

• | 4 Way M Metri-Pack 150 (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | DK BLU | 46 | Speaker Feed - Right Rear | A | DK BLU | 46 | Speaker Feed - Right Rear
B | LT BLU | 115 | Speaker Return - Right Rear | B | LT BLU | 115 | Speaker Return - Right Rear
C | BRN | 199 | Speaker Feed - Left Rear | C | BRN | 199 | Speaker Feed - Left Rear
D | YEL | 116 | Speaker Return - Left Rear | D | YEL | 116 | Speaker Return - Left Rear

#### C212 (Pontiac, Oldsmobile)

Connector Part Information |

• | 12052832

• | 2 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12052833

• | 2 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY | 118 | Speaker Return - Left Front (Olds, Buick) | A | GRY | 118 | Speaker Return - Left Front (Olds, Buick)
A | TAN | 201 | Speaker Feed - Left Front (Pontiac) | A | TAN | 201 | Speaker Feed - Left Front (Pontiac)
B | TAN | 201 | Speaker Feed - Left Front (Olds, Buick) | B | TAN | 201 | Speaker Feed - Left Front (Olds, Buick)
B | GRY | 118 | Speaker Return - Left Front (Pontiac) | B | GRY | 118 | Speaker Return - Left Front (Pontiac)

#### C301

Connector Part Information |

• | 12129081

• | 2 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129155

• | 2 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | DK GRN | 76 | Power Seat Motor Feed Passenger - Recline Fore | A | DK GRN | 76 | Power Seat Motor Feed Passenger - Recline Fore
B | DK BLU | 77 | Power Seat Motor Feed Passenger - Recline Aft | B | DK BLU | 77 | Power Seat Motor Feed Passenger - Recline Aft

#### C302

Connector Part Information |

• | 12129081

• | 2 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129082

• | 2 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 276 | Power Seat Motor Feed - Driver - Recline Fore | A | LT GRN | 276 | Power Seat Motor Feed - Driver - Recline Fore
B | LT BLU | 277 | Power Seat Motor Feed - Driver - Recline Aft | B | LT BLU | 277 | Power Seat Motor Feed - Driver - Recline Aft

#### C304

Connector Part Information |

• | 12064766

• | 8 Way F Metri-Pack 150 Series (BLU)

Connector Part Information

• | 12064767

• | 8 Way F Metri-Pack 150 Series (BLU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY | 8 | Instrument Panel Lamp Feed | A | GRY | 8 | Instrument Panel Lamp Feed
B | BLK | 1250 | Ground | B | BLK | 1250 | Ground
C | PNK | 739 | Fused Output - Ign 1 | C | PNK | 739 | Fused Output - Ign 1
D | DK GRN/WHT | 1135 | Brake Transmission Shift Interlock Solenoid Feed | D | DK GRN/WHT | 1135 | Brake Transmission Shift Interlock Solenoid Feed
E | ORN | 1732 | BCM Output - 12 V Inadvertent Load Control | E | ORN | 1732 | BCM Output - 12 V Inadvertent Load Control
F | TAN | 800 | Serial Data Signal UART | F | TAN | 800 | Serial Data Signal UART
G | PNK | 439 | Fused Output - Ign 1 | G | PNK | 439 | Fused Output - Ign 1
H | BLK/WHT | 451 | Ground | H | BLK/WHT | 451 | Ground

#### C312

Connector Part Information |

• | 12064749

• | 2 Way F Metri-Pack 480 Series (BLK)

Connector Part Information

• | 12066387

• | 2 Way M Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1340 | Fused Output - Bat | A | ORN | 1340 | Fused Output - Bat
B | BLK | 1250 | Ground | B | BLK | 1250 | Ground

#### C324 (Buick/Oldsmobile)

Connector Part Information |

• | 12064754

• | 6 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12064754

• | 6 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 282 | Power Seat Motor Feed - Driver - Rear Vertical Up | A | YEL | 282 | Power Seat Motor Feed - Driver - Rear Vertical Up
B | LT BLU | 283 | Power Seat Motor Feed - Driver - Rear Vertical Down | B | LT BLU | 283 | Power Seat Motor Feed - Driver - Rear Vertical Down
C | LT GRN | 284 | Power Seat Motor Feed - Driver - Horizontal Aft | C | LT GRN | 284 | Power Seat Motor Feed - Driver - Horizontal Aft
D | TAN | 285 | Power Seat Motor Feed - Driver Horizontal Fore | D | TAN | 285 | Power Seat Motor Feed - Driver Horizontal Fore
E | DK GRN | 286 | Power Seat Motor Feed - Driver - Front Vertical Up | E | DK GRN | 286 | Power Seat Motor Feed - Driver - Front Vertical Up
F | DK BLU | 287 | Power Seat Motor Feed - Driver - Front Vertical - Down | F | DK BLU | 287 | Power Seat Motor Feed - Driver - Front Vertical - Down

#### C326

Connector Part Information |

• | 12064754

• | 6 Way F Metri-Pack 280 Series (BLK

Connector Part Information

• | 12064754

• | 6 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 288 | Power Seat Motor Feed - Passenger - Rear Vertical Up | A | YEL | 288 | Power Seat Motor Feed - Passenger - Rear Vertical Up
B | LT BLU | 289 | Power Seat Motor Feed - Passenger - Rear Vertical Down | B | LT BLU | 289 | Power Seat Motor Feed - Passenger - Rear Vertical Down
C | LT GRN | 290 | Power Seat Motor Feed - Passenger - Rear Horizontal Aft | C | LT GRN | 290 | Power Seat Motor Feed - Passenger - Rear Horizontal Aft
D | TAN | 296 | Power Seat Motor Feed - Passenger - Rear Horizontal Fore | D | TAN | 296 | Power Seat Motor Feed - Passenger - Rear Horizontal Fore
E | DK GRN | 297 | Power Seat Motor Feed - Passenger - Front Vertical Up | E | DK GRN | 297 | Power Seat Motor Feed - Passenger - Front Vertical Up
F | DK BLU | 298 | Power Seat Motor Feed - Passenger - Front Vertical Down | F | DK BLU | 298 | Power Seat Motor Feed - Passenger - Front Vertical Down

#### C341

Connector Part Information |

• | 12047886

• | 8 Way F Metri-pack 150 Series (BLK)

Connector Part Information

• | 12045688

• | 8 Way Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT BLU | 1259 | Pneumatic Seat Soleniod Feed - Lower Lumbar - Passenger | A | LT BLU | 1259 | Pneumatic Seat Soleniod Feed - Lower Lumbar - Passenger
B | PNK | 1260 | Pneumatic Seat Solenoid Feed - Lumbar - Passenger | B | PNK | 1260 | Pneumatic Seat Solenoid Feed - Lumbar - Passenger
C | ORN | 1261 | Pneumatic Seat Solenoid Feed - Upper Lumbar - Passenger | C | ORN | 1261 | Pneumatic Seat Solenoid Feed - Upper Lumbar - Passenger
D | PNK | 1265 | Pneumatic Seat Solenoid Feed - Lateral - Passenger | D | PNK | 1265 | Pneumatic Seat Solenoid Feed - Lateral - Passenger
E | WHT | 766 | Pneumatic Seat Solenoid Feed - Coil - Driver - Inflate | E | WHT | 766 | Pneumatic Seat Solenoid Feed - Coil - Driver - Inflate
F | GRY | 764 | Pneumatic Seat Solenoid Feed - Coil - Driver - Deflate | F | GRY | 764 | Pneumatic Seat Solenoid Feed - Coil - Driver - Deflate
G | BLK | 769 | Pneumatic Seat Select Switch Output - Driver | G | BLK | 769 | Pneumatic Seat Select Switch Output - Driver
H | RED | 798 | Pneumatic Seat Solenoid Output - Passenger Seat | H | RED | 798 | Pneumatic Seat Solenoid Output - Passenger Seat

#### C345

Connector Part Information |

• | 12064749

• | 2 Way F Metri-Pack 480 Series (BLK)

Connector Part Information

• | 12064750

• | 2 Way M Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 1250 | Ground | A | BLK | 1250 | Ground
B | ORN | 1340 | Fused Output - Bat | B | ORN | 1340 | Fused Output - Bat

#### C350

Connector Part Information |

• | 12064763

• | 6 Way F Metri-Pack 150 Series (GRY)

Connector Part Information

• | 12064763

• | 6 Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TAN/WHT | 799 | Pneumatic Seat Solenoid Feed - Lower Lumbar - Driver | A | TAN/WHT | 789 | Pneumatic Seat Solenoid Feed - Lower Lumbar - Driver
B | BLK/WHT | 753 | Pneumatic Seat Solenoid Feed - Lumbar - Driver | B | BLK/WHT | 763 | Pneumatic Seat Solenoid Feed - Lumbar - Driver
C | YEL | 777 | Pneumatic Seat Solenoid Feed - Upper Lumbar - Driver | C | YEL | 777 | Pneumatic Seat Solenoid Feed - Upper Lumbar - Driver
D | PPL | 765 | Pneumatic Seat Solenoid Feed - Driver - Lateral | D | PPL | 765 | Pneumatic Seat Solenoid Feed - Driver - Lateral
E | -- | -- | Not Used | E | -- | -- | Not Used
F | TAN | 797 | Pneumatic Seat Solenoid Output - Driver seat | F | TAN | 797 | Pneumatic Seat Solenoid Output - Driver seat

#### C353

Connector Part Information |

• | 12064754

• | 6 Way M Metric -Pack 280 Series (BLK)

Connector Part Information

• | 12064752

• | 6 Way F Metric -Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | DK BLU | 298 | Power Seat Motor Feed, Passenger-Front Vertical Down | A | BLU | 298 | Power Seat Motor Feed, Passenger-Front Vertical Down
B | LT BLU | 289 | Power Seat Motor Feed, Passenger-Rear Vertical Down | B | LT BLU | 289 | Power Seat Motor Feed, Passenger-Rear Vertical Down
C | LT GRN | 290 | Power Seat Motor Feed, Passenger-Horizontal AFT | C | LT GRN | 290 | Power Seat Motor Feed, Passenger-Horizontal AFT
D | DK BLU | 1247 | Power Seat Motor Output-Passenger | D | DK GRN | 1247 | Power Seat Motor Output-Passenger
E | DK BLU | 77 | Power Seat Motor Feed Passenger-Recline AFT | E | DK GRN | 77 | Power Seat Motor Feed Passenger-Recline AFT
E | -- | -- | Not Used | F | -- | -- | Not Used

#### C400, C402

Connector Part Information |

• | 12047785

• | 4 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047786

• | 4 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | YEL | 18 | Stop/Turn Lamp Feed - Rear (LH) | B | YEL | 18 | Stop/Turn Lamp Feed - Rear (LH)
B | DK GRN | 19 | Stop/Turn Lamp Feed - Rear (RH) | B | DK GRN | 19 | Stop/Turn Lamp Feed - Rear (RH)
C | BLK | 1350 | Ground | C | BLK | 1250 | Ground

#### C401 (Oldsmobile)

Connector Part Information |

• | 12064760

• | 4 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12064761

• | 4 Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 9 | Park Lamp Feed | A | BRN | 9 | Park Lamp Feed
B | BLK | 1350 | Ground | B | BLK | 1350 | Ground
C | LT GRN | 24 | Back-up Lamp Feed | C | LT GRN | 24 | Back-up Lamp Feed
D | -- | -- | Not Used | D | -- | -- | Not Used

#### C401 (Pontiac)

Connector Part Information |

• | 12064760

• | 4 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12064761

• | 4 Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 9 | Park Lamp Feed (w/ UB3) | A | BRN/ WHT | 9 | Park Lamp Feed (w/ UB3)
A | PNK | 1255 | Park Lamp Feed - Side Marker/License- Monitored (w/ U50/U2F) | A | BRN/ WHT | 1255 | Park Lamp Feed - Side Marker/License- Monitored (w/ U50/U2F)
B | BLK | 1350 | Ground | B | LT BLU/WHT | 1350 | Ground
C | BRN | 9 | Park Lamp Feed (w/ UB3) | C | BRN | 9 | Park Lamp Feed (w/ UB3)
C | PNK | 1255 | Park Lamp Feed - Side Marker/License- Monitored (w/ U50/U2F) | C | PNK | 1255 | Park Lamp Feed - Side Marker/License- Monitored (w/ U50/U2F)
D | BLK | 1350 | Ground | D | BLK | 1350 | Ground

#### C406 (Pontiac)

Connector Part Information |

• | 12047781

• | 3 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047785

• | 3 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 9 | Park Lamp Feed (w/ UB3) | A | BRN | 9 | Park Lamp Feed (w/ UB3)
A | WHT | 1252 | Park Lamp Feed - Tail Lamps Monitored Group 2 (w/ U5O/U2F) | A | WHT | 1252 | Park Lamp Feed - Tail Lamps Monitored Group 2 (w/ U5O/U2F)
B | LT GRN | 24 | Back Up Lamp Feed (w/ UB3) | B | LT GRN | 24 | Back Up Lamp Feed (w/ UB3)
B | GRY | 1524 | Back Up Lamp Feed - Monitored (w/ U5O/U2F) | B | GRY | 1524 | Back Up Lamp Feed - Monitored (w/ U5O/U2F)
C | BLK | 1350 | Ground | C | BLK | 1350 | Ground

#### C410, C411

Connector Part Information |

• | 12047781

• | 3 Way M Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047782

• | 3 Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 18 | Stop/Turn Lamp Feed-Left Rear (LH) | A | YEL | 18 | Stop/Turn Lamp Feed-Left Rear (LH)
A | DK GRN | 19 | Stop/Turn Lamp Feed-Right Rear (RH) | A | DK GRN | 19 | Stop/Turn Lamp Feed-Right Rear (RH)
B | BRN | 9 | Park Lamp Feed | B | BRN | 9 | Park Lamp Feed
C | BLK | 1350 | Ground | C | BLK | 1350 | Ground

#### C415

Connector Part Information |

• | 12162143

• | 4 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12162102

• | 4 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 882 | Wheel Speed Sensor Signal - Right Rear | A | BLK | 882 | Wheel Speed Sensor Signal - Right Rear
B | WHT | 883 | Wheel Speed Sensor Return - Right Rear | B | WHT | 883 | Wheel Speed Sensor Return - Right Rear
C | BLK | 884 | Wheel Speed Sensor Signal - Left Rear | C | BLK | 884 | Wheel Speed Sensor Signal - Left Rear
D | WHT | 885 | Wheel Speed Sensor Return - Left Rear | D | WHT | 885 | Wheel Speed Sensor Return - Left Rear

#### C430, C431

Connector Part Information |

• | 12047781

• | 3 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047782

• | 3 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 9 | Park Lamp Feed | A | BRN | 9 | Park Lamp Feed
B | LT GRN | 24 | Back-up Lamp Feed | B | LT GRN | 24 | Back-up Lamp Feed
C | BLK | 1350 | Ground | C | BLK | 1350 | Ground

#### C440

Connector Part Information |

• | 12064752

• | 6 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12064754

• | 6 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RED | 1042 | Fused Output - Bat | A | RED | 1042 | Fused Output - Bat
B | BRN | 641 | Fused Output - Ign 3 | B | BRN | 641 | Fused Output - Ign 3
C | YEL | 321 | Electronic Level Control Relay Output Coil | C | YEL | 321 | Electronic Level Control Relay Output Coil
D | RED | 1042 | Fused Output - Bat | D | RED | 1042 | Fused Output - Bat
E | BLK | 1250 | Ground | E | BLK | 1250 | Ground
F | DK GRN | 322 | Electronic Level Control Compressor Motor Feed | F | DK GRN | 322 | Electronic Level Control Compressor Motor Feed

#### C501, C801 (Pontiac)

Connector Part Information |

• | 12059249

• | 2 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12059250

• | 2 Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1732 | BCM Output-12 V Inadvertent Load Control | A | ORN | 1732 | BCM Output-12 V Inadvertent Load Control
B | WHT | 156 | Courtesy Lamp Output | B | WHT | -- | Courtesy Lamp Output

#### C501, C801 (Buick/Oldsmobile)

Connector Part Information |

• | 12047785

• | 4 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12066498

• | 4 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1732 | BCM Output-12 V Inadvertent Load Control | A | ORN | 1732 | BCM Output-12 V Inadvertent Load Control
B | WHT | 156 | Courtesy Lamp Output | B | WHT | 156 | Courtesy Lamp Output
C-D | -- | -- | Not Used | C-D | -- | -- | Not Used

#### C502

Connector Part Information |

• | 12064752

• | 6 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12064754

• | 6 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TAN | 126 | Door Latch Switch Signal-Left Front | A | TAN | 126 | Door Latch Switch Signal-Left Front
B | -- | 745 | Door Ajar Switch Signal-Left Front | B | GRY/BLK | 745 | Door Ajar Switch Signal-Left Front
C | TAN | 694 | Power Door Lock Motor Feed-Driver Door Unlock | C | TAN | 694 | Power Door Lock Motor Feed-Driver Door Unlock
C | TAN | 294 | Power Door Lock Motor Feed-Driver Door Unlock(Oldsmobile w/o T2T, Buick w/o A62/AU0, Pontiac w/o AU0) | C | TAN | 294 | Power Door Lock Motor Feed-Driver Door Unlock(Oldsmobile w/o T2T, Buick w/o A62/AU0, Pontiac w/o AU0)
D | GRY | 295 | Power Door Lock Motor Feed-Lock | D | GRY | 295 | Power Door Lock Motor Feed-Lock
E | DK BLU/WHT | 727 | Door Latch Switch Signal-Secondary | E | DK BLU/WHT | 727 | Door Latch Switch Signal-Secondary
F | BLK | 1250 | Ground | F | BLK | 1250 | Ground

#### C601 (Oldsmobile, Buick)

Connector Part Information |

• | 12047785

• | 4 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12066498

• | 4 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1732 | BCM Output 12 V Inadvertant Load Control | A | ORN | 1732 | BCM Output 12 V Inadvertant Load Control
B | WHT | 156 | Courtesy Lamp Output | B | WHT | 156 | Courtesy Lamp Output
C-D | -- | -- | Not Used | C-D | -- | -- | Not Used

#### C601 (Pontiac)

Connector Part Information |

• | 12054244

• | 2 Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12052447

• | 2 Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1732 | BCM Output - 12 V - Inadvertant Load Control | A | ORN | 1732 | BCM Output - 12 V - Inadvertant Load Control
B | WHT | 156 | Courtesy Lamp Output | B | WHT | 156 | Courtesy Lamp Output

#### C602 (Pontiac) & C503

Connector Part Information |

• | 12047782

• | 3 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047781

• | 3 Way Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | BLK | 1250 | Ground | B | BLK | 1250 | Ground
C | LT GRN | 262 | Door Key Lock Cylinder Switch Signal Driver | C | LT GRN | 262 | Door Key Lock Cylinder Switch Signal Driver

#### C603

Connector Part Information |

• | 12064752

• | 6 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12064754

• | 6 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TAN | 1250 | Ground | A | BLK | 1250 | Ground
B | -- | -- | Not Used | B | -- | -- | Not Used
C | TAN | 294 | Power Door Lock Motor Feed-Unlock | C | TAN | 294 | Power Door Lock Motor Feed-Unlock
D | GRY | 295 | Power Door Lock Motor Feed-Lock | D | GRY | 295 | Power Door Lock Motor Feed-Lock
E | DK BLU/WHT | 746 | Door Ajar Switch Signal-Right Front | E | BLK/ WHT | 746 | Door Ajar Switch Signal-Right Front
F | BLK | 49 | Door Jamb Switch Signal Driver | F | DK BLU | 49 | Door Jamb Switch Signal Driver

#### C701

Connector Part Information |

• | 12047785

• | 4 Way F 150 Series Metri-Pack (BLK)

Connector Part Information

• | 12066498

• | 4 Way M 150 Series Metri-Pack (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1732 | BCM Output - 12 V - Inadvertant Load Control | A | ORN | 1732 | BCM Output - 12 V - Inadvertant Load Control
B | WHT | 156 | Courtesy Lamp Output | B | WHT | 156 | Courtesy Lamp Output
C | WHT | 156 | Courtesy Lamp Output | C | WHT | 156 | Courtesy Lamp Output
D | -- | -- | Not Used | D | -- | -- | Not Used

#### C702

Connector Part Information |

• | 12047785

• | 4 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047786

• | 4 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 1250 | Ground | A | BLK | 1250 | Ground
B | DK BLU | 49 | Door Jamb Switch Signal-Driver | B | WHT | 49 | Door Jamb Switch Signal-Driver
C | LT BLU/BLK | 747 | Door Ajar Switch Signal-Left Rear | C | BLK/YEL | 747 | Door Ajar Switch Signal-Left Rear
D | -- | -- | Not Used | D | -- | -- | Not Used

#### C703, C803

Connector Part Information |

• | 12064749

• | 2 Way F Metri-Pack 480 Series (BLK)

Connector Part Information

• | 12064750

• | 2 Way M Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TAN | 294 | Power Door Lock Motor Feed - Unlock | A | TAN | 294 | Power Door Lock Motor Feed - Unlock
B | GRY | 295 | Power Door Lock Motor Feed - Lock | B | GRY | 295 | Power Door Lock Motor Feed - Lock

#### C802

Connector Part Information |

• | 12047785

• | 4 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12066498

• | 4 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | DK BLU | 49 | Door Jamb Switch - Driver | A | DK BLU | 49 | Door Jamb Switch - Driver
B | BLK | 1250 | Ground | B | BLK | 1250 | Ground
C | -- | -- | Not Used | C | -- | -- | Not Used
D | LT BLU | 74 | Park Lamp Switch Output | D | LT BLU | 74 | Park Lamp Switch Output