For 1990-2009 cars

### Removal Procedure

1. Remove the IP cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .
2. Remove the instrument cluster lens fasteners to the instrument cluster, if necessary.
3. Release the instrument cluster lens retainers, if necessary.
4. Remove the instrument cluster lens.

### Installation Procedure

Ensure the instrument cluster lens surface is completely clean before assembly.

1. Install the instrument cluster lens to the instrument cluster.
2. Carefully push inward on the outside of the lens in order to fasten the lens retainers, if necessary.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the instrument cluster lens fasteners to the instrument cluster, if necessary.

Tighten
Tighten the fasteners to 1.9 N·m (17 lb in).

4. Install the IP cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .