For 1990-2009 cars

• | If abnormal noise exists in the front end, inspect for the following conditions:

- | Inadequate lubrication of ball joints and tie rod ends

- | Damaged strut or mountings

- | Worn tie rod ends

- | Worn control arm bushings

- | Loose stabilizer shaft

- | Loose wheel nuts

- | Loose suspension mounting bolts

- | Loose mounts

- | Noisy wheel covers

- | Incorrect rack bearing preload

- | Tire noise

• | Inspect for diagnostic trouble codes in the computer command ride system.