For 1990-2009 cars

### Removal Procedure

1. Disengage the retainers on the back side of the molding (1).
2. Remove the windshield pillar garnish molding (1).

### Installation Procedure

1. Connect the new fasteners (2) to the windshield pillar garnish molding (1) if they are broken or damaged.
2. Align the fasteners (2) to the holes in the windshield pillar.
3. Press the windshield pillar garnish molding (1) into place.