For 1990-2009 cars

If wander or poor steering stability exists, inspect for the following conditions:

• | Mismatched or uneven tires

• | Incorrect front or rear wheel alignment

• | Inadequate lubrication of ball joints or tie rod ends

• | Worn tie rod ends

• | Worn ball joints

• | Worn strut dampers

• | Broken or sagging springs

• | Loose stabilizer shaft

• | Incorrect power steering fluid pressure

• | Loose rack and pinion gear attaching bolts

• | Worn or binding rack and pinion gear

• | Worn steering column friction damper