For 1990-2009 cars

Table 1: | Warning/Staus Message List
Table 2: | Lamp Monitor Bulb Usage

The driver information center (DIC) is a 2 color vacuum fluorescent (VF) display that contains the following information:

• | The odometers

• | The warning indicators

• | The lamp monitor displays

• | A graphic representation of the vehicle

#### Warning/Staus Message List

Fault | Illuminated Segments
--- | ---
No Fault | Vehicle Outline
Low Coolant | Vehicle Outline, Engine, LOW COOLANT
Low Fuel | Vehicle Outline, Fuel Tank, CHECK GAUGES
Low Washer Fluid | Vehicle Outline, WASHER FLUID, Windshield (Flashes 5 times, then stays ON)
Low Oil Level | Vehicle Outline, Engine, CHECK OIL LEVEL
Low Oil Pressure | Vehicle Outline, Engine, CHECK GAUGES
Low or High Voltage | Vehicle Outline, Engine, CHECK GAUGES
High Coolant Temperature | Vehicle Outline, Engine, Check Gauges
Trunk Ajar | Vehicle Outline, Trunk, TRUCK AJAR
Hood Ajar | Vehicle Outline, Hood, HOOD AJAR
Door Ajar | Vehicle Outline, DOOR AJAR, Corresponding Door
Front Park Lamp Failure | Vehicle Outline, Front Lamps, LAMP MONITOR, PARK LAMP
Headlamp Failure | Vehicle Outline, Front Lamps, LAMP MONITOR, HEAD LAMP
High-Beam Failure | Vehicle Outline, Front Lamps, LAMP MONITOR, HI BEAM LAMP
Front Turn Signal Failure | Vehicle Outline, Front Lamps, LAMP MONITOR, TURN SIGNAL LAMP
Tail Lamp Failure | Vehicle Outline, Rear Lamps, LAMP MONITOR, TAIL LAMP
Backup Lamp Failure | Vehicle Outline, Rear Lamps, LAMP MONITOR, BACKUP LAMP
License Plate Lamp Failure | Vehicle Outline, Rear Lamps, LAMP MONITOR, TAIL LAMP
Rear Turn Signal Failure | Vehicle Outline, Rear Lamps, LAMP MONITOR, TURN SIGNAL LAMP
Brake Lamp Failure | Vehicle Outline, Rear Lamps, LAMP MONITOR, BRAKE LAMP
CHMSL Failure | Vehicle Outline, CHMSL, LAMP MONITOR, BRAKE LAMP
Lamp Monitor | Vehicle Outline, LAMP MONITOR

### Lamp Monitor Bulb Usage Table

Important: When replacing a bulb, replace the bulb with the same type. If you use the incorrect bulb type, the DIC will continue to display a bulb outage.

Follow the chart below before proceeding with the diagnosis.

If the bulb indicator outages are displayed on the driver information center (DIC), follow the chart below in order to determine if a bulb is burnt out. Also verify proper bulb type.

#### Lamp Monitor Bulb Usage

Indicator | Bulbs to Test
--- | ---
The high beam indicator turns on. | The 2 high beam bulbs
The low beam indicator turns on. | The 2 low beam bulbs
The park lamp turns on. |

• | The left side:

- | The 1 park/turn bulb

- | The 1 side marker bulb

• | The right side:

- | The 1 park/turn bulb

- | The 1 side marker bulb

The turn lamps turn on. | The 4 turn signal bulbs:

• | The left side front bulb

• | The right side front bulb

• | The left side rear bulb

• | The right side rear bulb

The taillamp indicator turns on. |

• | The 4 tail bulbs:

- | The 2 left bulbs

- | The 2 right bulbs

• | The 2 license bulbs

• | The 4 tail/turn/stop bulbs

• | The 2 rear side marker bulbs:

- | The 1 left bulb

- | The 1 right bulb

The backup indicator turns on. | The 2 backup bulbs
The brake lamp indicator turns on. |

1. The 4 stop/turn tail bulbs
2. The 1 CHMSL bulb

The taillamp indicator and the brake indicator turn on together. | The 4 stop/turn/tail bulbs:

• | The 2 left bulbs

• | The 2 right bulbs