For 1990-2009 cars

## Instrument Panel Accessory Trim Plate Replacement Oldsmobile

### Removal Procedure

1. Remove the IP trim plate. Refer to Instrument Panel Lower Center Trim Replacement .
2. Remove the fasteners (2) from the IP center air outlet deflector housing trim plate.
3. Pull the trim plate rearward carefully to disengage the trim plate retaining clips (1).

Remove the trim plate.

### Installation Procedure

1. Align the IP center air outlet deflector housing trim plate retaining clips (1) to the IP.

Push inward in order to secure the trim plate.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the trim plate fasteners (2).

Tighten
Tighten the trim plate fasteners to 1.9 N·m (17 lb in).

3. Install the IP trim plate. Refer to Instrument Panel Lower Center Trim Replacement .