For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Tire and Wheel Assembly Runout (Radial and Lateral)
Off-Vehicle | 1.27 mm | 0.050 in
On-Vehicle | 1.52 mm | 0.060 in
Steel Wheel Runout
Radial | 1.01 mm | 0.040 in
Lateral | 1.14 mm | 0.045 in
Aluminum Wheel Runout
Radial | 0.76 mm | 0.030 in
Lateral | 0.76 mm | 0.030 in
Wheel Stud Runout | 0.25 mm | 0.010 in
Wheel Hub/Axle Flange Runout | 0.132 mm | 0.0052 in