For 1990-2009 cars

# DRIVEABILITY SYMTOMS MAYBE OPERATING IAC

#### VEHICLES AFFECTED: 1988-1989 A,C,E,H,AND N, 3300,3800 ENGINES

This bulletin cancels and replaces previous Bulletin due to new procedures.

We have recently seen a few cases of internally shorted Idle Air Control Motor terminals on 1988 and 1989 models equipped with 3800 engines, and 1989 models equipped with 3300 engines, which may exhibit one or more of a variety of poor driveability conditions. Some of those conditions could include:

1. Engine miss at idle or rough idle (engine can be hot or cold). 2. Engine miss under light acceleration. 3. General engine roughness at all engine speeds. 4. Cycling whine (generator) accompanied by fluctuating RPM at idle (3 or 4 times at each stop). 5. Chuggle at approximately 27 kph (45 mph.). 6. Excessive rattle from EGR valve (some noise, is normal). 7. Transmission comments about 3-4 shifts (rough or repetitive 4th gear engagements). 8. Comments about T.C.C. operation (rough, shudder).

It should be noted that each vehicle may exhibit different symptoms and these sometimes can be intermittent. Although this condition is not very wide spread, it can be very difficult to diagnose unless the following procedure is used, since an IAC motor is not generally associated with these types of comments.

A quick test of the IAC motor can be performed by simply disconnecting the harness connector at the IAC motor and determining if the poor driveability condition is eliminated or not. The harness should be disconnected with the engine running and the IAC motor counts stabilized.

If the symptoms are still present with the IAC motor disconnected, DO NOT REPLACE THE IAC MOTOR. At this point, it will be necessary to reconnect the IAC motor and refer to the appropriate Chassis Service Manual for further diagnostics.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.