For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the negative battery cable. Refer to Battery.
3. Remove the right dash panel sound insulator. Refer to Instrument Panel, Guages, and Console.
4. Remove the relay electrical center cover.
5. Remove the fuel pump relay (2) from the right half I/P Power Distribution Center (1).

### Installation Procedure

1. Install the fuel pump relay (2) into the right half Instrument Panel Power Distribution Center (1).
2. Install the relay electrical center cover.
3. Install the right dash panel sound insulator. Refer to Instrument Panel, Guages, and Console.
4. Turn the ignition OFF.
5. Install the negative battery cable. Refer to Battery.