For 1990-2009 cars

#### Tools Required

J 36850 Assembly Lubricant

1. Install a new O-ring seal (36) onto the electrical connector assembly (35). Lubricate with J 36850 or equivalent.
2. Install the electrical connector assembly (35) into the case. Lubricate with J 36850 or equivalent.
3. Use a hammer and a punch in order to install the vent assembly (37), if necessary.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the oil pressure test hole plug (38).

Tighten
Tighten the test hold plug to 11 N·m (97 lb in).